(kicad_pcb (version 4) (host pcbnew "(2015-05-16 BZR 5655)-product")
  (general
    (links 0)
    (no_connects 0)
    (area 99.924999 33.4775 150.075001 85.6975)
    (thickness 1.6)
    (drawings 5)
    (tracks 27)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 4.5 3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module mycomponents:SMA_SIDE (layer F.Cu) (tedit 5570B61C)
    (at 107.3 38.5)
    (fp_text reference P1 (at 0 3.2) (layer F.SilkS) hide)
    (fp_text value BNC (at -0.3 -4.5) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 5) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -3.5 0) (size 3 5) (layers *.Mask B.Cu))
    (pad 2 smd rect (at 3.5 0) (size 3 5) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 3.5 0) (size 3 5) (layers *.Mask B.Cu))
    (pad 2 smd rect (at -3.5 0) (size 3 5) (layers F.Cu F.Mask))
    (model lib/SMA_EDGE.wrl
      (at (xyz -0 0.15 0.063))
      (scale (xyz 1.27 1.27 1.27))
      (rotate (xyz 90 0 90))
    )
  )
  (module mycomponents:SMA_SIDE (layer F.Cu) (tedit 551AFA2F)
    (at 107.6 81.45)
    (fp_text reference P1 (at 0 3.2) (layer F.SilkS) hide)
    (fp_text value BNC (at 0 3.8) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 5) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -3.5 0) (size 3 5) (layers *.Mask B.Cu))
    (pad 2 smd rect (at 3.5 0) (size 3 5) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 3.5 0) (size 3 5) (layers *.Mask B.Cu))
    (pad 2 smd rect (at -3.5 0) (size 3 5) (layers F.Cu F.Mask))
    (model lib/SMA_EDGE.wrl
      (at (xyz -0 0.15 0.063))
      (scale (xyz 1.27 1.27 1.27))
      (rotate (xyz 90 0 90))
    )
  )
  (gr_text "1420 MHz bandpass\nSven Brauch 2015" (at 127.85 40.25) (layer F.Cu))
  (gr_line (start 101 85) (end 101 35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150 84) (end 100 84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149 35) (end 149 85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 36) (end 150 36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.4 70.25) (xy 142.6 73.05) (xy 114.6 73.05) (xy 113.1 73.05) (xy 113.1 70.25)
        (xy 114.6 70.25) (xy 142.6 70.25) (xy 142.6 68.25) (xy 114.6 68.25) (xy 113.1 68.25)
        (xy 113.1 65.45) (xy 114.6 65.45) (xy 142.6 65.45) (xy 145.4 68.25) (xy 145.4 70.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.1 64.15) (xy 142.6 64.15) (xy 114.6 64.15) (xy 111.8 61.35) (xy 111.8 59.35)
        (xy 114.6 56.55) (xy 142.6 56.55) (xy 144.1 56.55) (xy 144.1 59.35) (xy 142.6 59.35)
        (xy 114.6 59.35) (xy 114.6 61.35) (xy 142.6 61.35) (xy 144.1 61.35) (xy 144.1 64.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.4 52.45) (xy 142.6 55.25) (xy 114.6 55.25) (xy 113.1 55.25) (xy 113.1 52.45)
        (xy 114.6 52.45) (xy 142.6 52.45) (xy 142.6 50.45) (xy 114.6 50.45) (xy 113.1 50.45)
        (xy 113.1 47.65) (xy 114.6 47.65) (xy 142.6 47.65) (xy 145.4 50.45) (xy 145.4 52.45)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.6 75.1) (xy 108.5 75.1) (xy 108.5 79) (xy 106.75 79) (xy 106.75 75.1)
        (xy 107.65 74.2) (xy 108.5 73.3) (xy 142.6 73.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.6 47.4) (xy 108.25 47.4) (xy 107.35 46.45) (xy 106.5 45.6) (xy 106.5 40.6)
        (xy 108.25 40.6) (xy 108.25 45.6) (xy 142.6 45.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101 36) (xy 149 36) (xy 149 84) (xy 101 84)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101 36) (xy 149 36) (xy 149 84) (xy 101 84)
      )
    )
  )
)
