(kicad_pcb (version 3) (host pcbnew "(2013-may-18)-stable")
  (general
    (links 34)
    (no_connects 2)
    (area 96.1316 65.802688 145.0684 88.315001)
    (thickness 1.6)
    (drawings 6)
    (tracks 72)
    (zones 0)
    (modules 17)
    (nets 12)
  )
  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.254)
    (zone_clearance 0.8)
    (zone_45_only yes)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (user_via 2.2 1)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 3178497)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 2)
      (mirror true)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory /tmp))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 N-0000010)
  (net 3 N-0000011)
  (net 4 N-000004)
  (net 5 N-000005)
  (net 6 N-000006)
  (net 7 N-000007)
  (net 8 N-000008)
  (net 9 N-000009)
  (net 10 VCC)
  (net 11 VDD)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net GND)
    (add_net N-0000010)
    (add_net N-0000011)
    (add_net N-000004)
    (add_net N-000005)
    (add_net N-000006)
    (add_net N-000007)
    (add_net N-000008)
    (add_net N-000009)
    (add_net VCC)
    (add_net VDD)
  )
  (module Vishay_LED (layer F.Cu) (tedit 50B54A6C)
    (at 109.4 76.4 180)
    (fp_text reference D1 (at 0 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.19888 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45034 0 180) (size 1.69926 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 6 N-000006)
    )
    (pad 2 smd rect (at 1.45034 0 180) (size 1.69926 2.70002)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
  )
  (module SMA_SIDE (layer F.Cu) (tedit 53CD5082)
    (at 137.4 81.4 90)
    (fp_text reference P3 (at 0.1 4.3 90) (layer F.SilkS))
    (fp_text value BNC (at 0.1 6.5 90) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 90) (size 2.5 5)
      (layers F.Cu F.Paste F.Mask)
      (net 5 N-000005)
    )
    (pad 2 smd rect (at -3.5 0 90) (size 3 5)
      (layers B.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 2 smd rect (at 3.5 0 90) (size 3 5)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 2 smd rect (at 3.5 0 90) (size 3 5)
      (layers B.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 2 smd rect (at -3.5 0 90) (size 3 5)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
  )
  (module SMA_SIDE (layer F.Cu) (tedit 53CD5082)
    (at 103.8 81.4 270)
    (fp_text reference P2 (at 0.1 4.3 270) (layer F.SilkS))
    (fp_text value BNC (at 0.1 6.5 270) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 270) (size 2.5 5)
      (layers F.Cu F.Paste F.Mask)
      (net 2 N-0000010)
    )
    (pad 2 smd rect (at -3.5 0 270) (size 3 5)
      (layers B.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 2 smd rect (at 3.5 0 270) (size 3 5)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 2 smd rect (at 3.5 0 270) (size 3 5)
      (layers B.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 2 smd rect (at -3.5 0 270) (size 3 5)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
  )
  (module SM0603_Resistor (layer F.Cu) (tedit 5051B21B)
    (at 126.2 82.1 90)
    (attr smd)
    (fp_text reference R6 (at 0.0635 -0.0635 180) (layer F.SilkS))
    (fp_text value 500 (at -1.69926 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 8 N-000008)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000009)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Resistor (layer F.Cu) (tedit 5051B21B)
    (at 118.4 86.6)
    (attr smd)
    (fp_text reference R5 (at 0.0635 -0.0635 90) (layer F.SilkS))
    (fp_text value 10 (at -1.69926 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 7 N-000007)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 8 N-000008)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Resistor (layer F.Cu) (tedit 5051B21B)
    (at 114.4 80.6 270)
    (attr smd)
    (fp_text reference R3 (at 0.0635 -0.0635 360) (layer F.SilkS))
    (fp_text value 2k2 (at -1.69926 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 11 VDD)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 3 N-0000011)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Resistor (layer F.Cu) (tedit 5051B21B)
    (at 116.4 80.6 90)
    (attr smd)
    (fp_text reference R4 (at 0.0635 -0.0635 180) (layer F.SilkS))
    (fp_text value 2k2 (at -1.69926 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 3 N-0000011)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Resistor (layer F.Cu) (tedit 5051B21B)
    (at 108.8 82.2 270)
    (attr smd)
    (fp_text reference R1 (at 0.0635 -0.0635 360) (layer F.SilkS))
    (fp_text value 50R (at -1.69926 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 2 N-0000010)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Resistor (layer F.Cu) (tedit 5051B21B)
    (at 132.8 81.3)
    (attr smd)
    (fp_text reference R7 (at 0.0635 -0.0635 90) (layer F.SilkS))
    (fp_text value 50R (at -1.69926 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 N-000004)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 5 N-000005)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Resistor (layer F.Cu) (tedit 5051B21B)
    (at 113.6 76.4 180)
    (attr smd)
    (fp_text reference R2 (at 0.0635 -0.0635 270) (layer F.SilkS))
    (fp_text value 2k2 (at -1.69926 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 11 VDD)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 6 N-000006)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 115 86.6)
    (attr smd)
    (fp_text reference C3 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 7 N-000007)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 111.6 81.4)
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 2 N-0000010)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 3 N-0000011)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 129.8 81.3)
    (attr smd)
    (fp_text reference C4 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000009)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 N-000004)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 112.6 71.8 270)
    (attr smd)
    (fp_text reference C1 (at 0 0 360) (layer F.SilkS))
    (fp_text value 2.2uF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 10 VCC)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module DPAK3 (layer F.Cu) (tedit 42808881)
    (at 120.2 73 270)
    (tags "CMS DPACK")
    (fp_text reference U1 (at 0 -14.224 270) (layer F.SilkS))
    (fp_text value MC78M05 (at 0 -3.302 270) (layer F.SilkS))
    (pad 2 smd rect (at 0 -8.763 270) (size 10.668 8.89)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 2 smd rect (at 0 0 270) (size 1.778 2.286)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 1 smd rect (at -2.54 0 270) (size 1.778 2.286)
      (layers F.Cu F.Paste F.Mask)
      (net 10 VCC)
    )
    (pad 3 smd rect (at 2.54 0 270) (size 1.778 2.286)
      (layers F.Cu F.Paste F.Mask)
      (net 11 VDD)
    )
    (model smd/dpack_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 2pin_2.54mm (layer F.Cu) (tedit 516095F4)
    (at 115.8 71.8 90)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P1 (at 0 -3.048 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 2.794 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.30048 0 90) (size 2 3) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 GND)
    )
    (pad 2 thru_hole rect (at 1.30048 0 270) (size 2 3) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 VCC)
    )
  )
  (module SOT23-5 (layer F.Cu) (tedit 4ECF78EF)
    (at 120.2 82.6 180)
    (attr smd)
    (fp_text reference U2 (at 2.19964 -0.29972 270) (layer F.SilkS))
    (fp_text value LMH6723MF (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 1.27 180) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000009)
    )
    (pad 3 smd rect (at 0.9525 1.27 180) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 3 N-0000011)
    )
    (pad 5 smd rect (at -0.9525 -1.27 180) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 11 VDD)
    )
    (pad 2 smd rect (at 0 1.27 180) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 4 smd rect (at 0.9525 -1.27 180) (size 0.508 0.762)
      (layers F.Cu F.Paste F.Mask)
      (net 8 N-000008)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 100.965 67.945) (end 100.965 67.31) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.965 67.31) (end 100.965 67.945) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.335 67.31) (end 100.965 67.31) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.335 88.265) (end 140.335 67.31) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.965 88.265) (end 140.335 88.265) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.965 67.945) (end 100.965 88.265) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.5)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.2))
    (polygon
      (pts
        (xy 140.335 88.265) (xy 100.965 88.265) (xy 100.965 67.31) (xy 140.335 67.31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.2))
    (polygon
      (pts
        (xy 118.8 75) (xy 117.2 75) (xy 117.2 71.4) (xy 118.8 71.4)
      )
    )
  )
)
