(kicad_pcb (version 4) (host pcbnew "(2015-07-13 BZR 5935)-product")
  (general
    (links 43)
    (no_connects 0)
    (area 149.849999 95.2775 189.050001 122.775)
    (thickness 1.6)
    (drawings 10)
    (tracks 241)
    (zones 0)
    (modules 23)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.45 0.3)
    (user_via 1.2 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 GND)
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "Net-(C7-Pad2)")
  (net 9 "Net-(C8-Pad1)")
  (net 10 VCC)
  (net 11 "Net-(D1-Pad1)")
  (net 12 "Net-(R5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 157 107.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.6) (layer F.SilkS))
    (fp_text value 16pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5571A536)
    (at 158.8 111.7)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.4 0) (layer F.SilkS))
    (fp_text value 12pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5571A54D)
    (at 161.2 112.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.4 0 270) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5571A570)
    (at 167.3 112.7 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.5 -0.1 270) (layer F.SilkS))
    (fp_text value 12pF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5571A57A)
    (at 167 105)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.6) (layer F.SilkS))
    (fp_text value 8.2pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5571A60F)
    (at 184.5 117.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 2.5 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5571A612)
    (at 184.5 118.9)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.5 0) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5571A5EE)
    (at 177.2 119.9)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 3 0) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5571A650)
    (at 165 118.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D1 (at 2.3 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SMA_SIDE (layer F.Cu) (tedit 551AFA2F)
    (at 170.3 99.6 180)
    (fp_text reference P1 (at 0 3.2 180) (layer F.SilkS) hide)
    (fp_text value BNC (at 0 3.8 180) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 2.5 5) (layers F.Cu F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at -3.5 0 180) (size 3 5) (layers *.Mask B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 3.5 0 180) (size 3 5) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 3.5 0 180) (size 3 5) (layers *.Mask B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -3.5 0 180) (size 3 5) (layers F.Cu F.Mask)
      (net 4 GND))
    (model lib/SMA_EDGE.wrl
      (at (xyz -0 0.15 0.063))
      (scale (xyz 1.27 1.27 1.27))
      (rotate (xyz 90 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5571A53A)
    (at 158.8 113.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.3 0) (layer F.SilkS))
    (fp_text value 100R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5571A575)
    (at 169.8 107.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.6 270) (layer F.SilkS))
    (fp_text value 100R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5571A550)
    (at 162.8 111.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.3 0.1 270) (layer F.SilkS))
    (fp_text value 220R (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5571A555)
    (at 165.1 111.9)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.6) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5571A578)
    (at 163.5 105)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0.1 -1.6) (layer F.SilkS))
    (fp_text value 5 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5571A573)
    (at 169.5 111.9)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.6) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5571A641)
    (at 163 118.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.3 -0.1 270) (layer F.SilkS))
    (fp_text value 2200 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINHEAD1-2 (layer F.Cu) (tedit 0)
    (at 158.5 118.5 90)
    (attr virtual)
    (fp_text reference P2 (at 0 -3.9 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -1.27 0 90) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 10 VCC))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module mycomponents:SMA_SIDE (layer F.Cu) (tedit 5571B639)
    (at 152.6 107.1 90)
    (fp_text reference IN1 (at 0 3.2 90) (layer F.SilkS) hide)
    (fp_text value BNC (at 0 3.8 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 0 90) (size 2.5 5) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -3.5 0 90) (size 3 5) (layers *.Mask B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 3.5 0 90) (size 3 5) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 3.5 0 90) (size 3 5) (layers *.Mask B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -3.5 0 90) (size 3 5) (layers F.Cu F.Mask)
      (net 4 GND))
    (model lib/SMA_EDGE.wrl
      (at (xyz -0 0.15 0.063))
      (scale (xyz 1.27 1.27 1.27))
      (rotate (xyz 90 0 90))
    )
  )
  (module mycomponents:TO252 (layer F.Cu) (tedit 5571B90E)
    (at 178 117.5)
    (fp_text reference U1 (at -2.6 -11.5) (layer F.SilkS))
    (fp_text value 78L05 (at 0 -9.5) (layer F.SilkS) hide)
    (pad GND smd rect (at 0 -6.9) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad VO smd rect (at 2.3 0) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad VI smd rect (at -2.3 0) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
  )
  (module mycomponents:3.5nH-microstrip (layer F.Cu) (tedit 5571BA19)
    (at 157.9 109.5)
    (solder_mask_margin 0.01)
    (clearance 0.01)
    (fp_text reference L1 (at 3.025 0 90) (layer F.SilkS) hide)
    (fp_text value 3.5nH (at 0 -5.5) (layer F.Fab))
    (pad 1 smd rect (at 0.575 -1.2) (size 1.15 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -0.575 1.2) (size 1.15 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad ~ smd rect (at 1.15 -0.9) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 1.15 0.3) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 0 -0.6) (size 2.3 0.3) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 0 0) (size 2.3 0.3) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 0 0.6) (size 2.3 0.3) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at -1.15 -0.3) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at -1.15 0.9) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask))
  )
  (module mycomponents:3.5nH-microstrip (layer F.Cu) (tedit 5571BA19)
    (at 166 108.4 180)
    (solder_mask_margin 0.01)
    (clearance 0.01)
    (fp_text reference L2 (at 3.025 0 270) (layer F.SilkS) hide)
    (fp_text value 3.5nH (at 0 -5.5 180) (layer F.Fab))
    (pad 1 smd rect (at 0.575 -1.2 180) (size 1.15 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at -0.575 1.2 180) (size 1.15 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad ~ smd rect (at 1.15 -0.9 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 1.15 0.3 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 0 -0.6 180) (size 2.3 0.3) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 0 0 180) (size 2.3 0.3) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at 0 0.6 180) (size 2.3 0.3) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at -1.15 -0.3 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask))
    (pad ~ smd rect (at -1.15 0.9 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask))
  )
  (module mycomponents:SOT343-AVAGO (layer F.Cu) (tedit 5571BB92)
    (at 160 106 180)
    (fp_text reference T1 (at -0.65 2.55 180) (layer F.SilkS))
    (fp_text value ATF54143 (at 3 -3.75 180) (layer F.Fab))
    (pad 3 smd rect (at 0.65 -1 180) (size 0.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -0.65 -1 180) (size 0.6 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.65 1 180) (size 0.6 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.5 1 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (gr_text "1420 MHz LNA\nSven Brauch 2015" (at 185.5 108 270) (layer F.SilkS))
  (gr_text "-\n+" (at 152 118.25) (layer F.SilkS))
  (gr_line (start 150 122) (end 150 97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189 122) (end 150 122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189 97) (end 189 122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 97) (end 189 97) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.0001)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.2 106.8) (xy 167.8 106.8) (xy 167.8 110) (xy 164.2 110)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.0001)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.1 106.7) (xy 156.7 106.7) (xy 156.7 107.5) (xy 155.1 107.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.0001)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.6 111.1) (xy 158.4 111.1) (xy 158.4 111.4) (xy 157.7 111.4) (xy 157.7 111.1)
        (xy 156.1 111.1) (xy 156.1 108) (xy 156.3 108) (xy 157.3 108) (xy 157.3 107.5)
        (xy 157.3 106.7) (xy 159.1 106.7) (xy 159.1 107.5) (xy 158.2 107.5) (xy 158.2 108)
        (xy 159.6 108) (xy 159.6 111) (xy 159.6 111.1)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1.75))
    (polygon
      (pts
        (xy 150 97) (xy 189 97) (xy 189 122) (xy 150 122)
      )
    )
  )
)
