(kicad_pcb (version 4) (host pcbnew "(2015-10-16 BZR 6271)-product")
  (general
    (links 448)
    (no_connects 0)
    (area 176.5 110.787 283.101381 162.48)
    (thickness 1.6)
    (drawings 142)
    (tracks 3267)
    (zones 0)
    (modules 190)
    (nets 217)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (1 Inner2.Cu signal hide)
    (2 Inner1.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (user_trace_width 1.5)
    (trace_clearance 0.175)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.175)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.453)
    (via_min_drill 0.3)
    (user_via 0.46 0.3)
    (user_via 0.7 0.5)
    (user_via 1.2 0.7)
    (uvia_size 0.2)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.1)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x010f8_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 +5V)
  (net 3 ADC_CLOCK)
  (net 4 ATT1_SWITCH_A)
  (net 5 ATT1_SWITCH_B)
  (net 6 CP_OUT)
  (net 7 GND)
  (net 8 IF_AFTER_AMP1)
  (net 9 IF_AFTER_AMP2)
  (net 10 IF_AFTER_ATT1)
  (net 11 IF_AFTER_FILTER)
  (net 12 IF_AFTER_PREAMP)
  (net 13 IF_AFTER_SAW)
  (net 14 IF_FILTERED)
  (net 15 IF_RAW)
  (net 16 LO_CLOCK)
  (net 17 LO_LOCK_DETECT)
  (net 18 LO_RAW)
  (net 19 LO_SPI_CLOCK)
  (net 20 LO_SPI_DATA)
  (net 21 LO_SPI_LE)
  (net 22 RST)
  (net 23 SKY)
  (net 24 USB_BOOT)
  (net 25 VCC)
  (net 26 V_TUNE)
  (net 27 "Net-(B1-Pad3)")
  (net 28 "Net-(B1-Pad4)")
  (net 29 "Net-(B1-Pad6)")
  (net 30 "Net-(B2-Pad1)")
  (net 31 "Net-(B2-Pad3)")
  (net 32 "Net-(C1-Pad2)")
  (net 33 "Net-(C3-Pad1)")
  (net 34 "Net-(C3-Pad2)")
  (net 35 "Net-(C4-Pad1)")
  (net 36 "Net-(C5-Pad1)")
  (net 37 "Net-(C6-Pad2)")
  (net 38 "Net-(C10-Pad2)")
  (net 39 "Net-(C11-Pad1)")
  (net 40 "Net-(C13-Pad1)")
  (net 41 "Net-(C15-Pad1)")
  (net 42 "Net-(C17-Pad1)")
  (net 43 "Net-(C18-Pad1)")
  (net 44 "Net-(C18-Pad2)")
  (net 45 "Net-(C20-Pad1)")
  (net 46 "Net-(C24-Pad1)")
  (net 47 "Net-(C28-Pad1)")
  (net 48 "Net-(C32-Pad1)")
  (net 49 "Net-(C34-Pad1)")
  (net 50 "Net-(C34-Pad2)")
  (net 51 "Net-(C36-Pad1)")
  (net 52 "Net-(C38-Pad2)")
  (net 53 "Net-(C39-Pad2)")
  (net 54 "Net-(C41-Pad1)")
  (net 55 "Net-(C45-Pad1)")
  (net 56 "Net-(C47-Pad2)")
  (net 57 "Net-(C48-Pad2)")
  (net 58 "Net-(C50-Pad1)")
  (net 59 "Net-(C51-Pad1)")
  (net 60 "Net-(C51-Pad2)")
  (net 61 "Net-(C52-Pad1)")
  (net 62 "Net-(C53-Pad1)")
  (net 63 "Net-(C53-Pad2)")
  (net 64 "Net-(C54-Pad1)")
  (net 65 "Net-(C54-Pad2)")
  (net 66 "Net-(C55-Pad1)")
  (net 67 "Net-(C56-Pad2)")
  (net 68 "Net-(C58-Pad1)")
  (net 69 "Net-(C61-Pad1)")
  (net 70 "Net-(C61-Pad2)")
  (net 71 "Net-(C62-Pad1)")
  (net 72 "Net-(C78-Pad2)")
  (net 73 "Net-(C79-Pad2)")
  (net 74 "Net-(C80-Pad2)")
  (net 75 "Net-(CON1-Pad1)")
  (net 76 "Net-(D2-Pad2)")
  (net 77 "Net-(D3-Pad2)")
  (net 78 "Net-(D4-Pad2)")
  (net 79 "Net-(D5-Pad1)")
  (net 80 "Net-(D5-Pad2)")
  (net 81 "Net-(D6-Pad1)")
  (net 82 "Net-(D6-Pad2)")
  (net 83 "Net-(FB2-Pad2)")
  (net 84 "Net-(L6-Pad2)")
  (net 85 "Net-(P2-Pad2)")
  (net 86 "Net-(P2-Pad4)")
  (net 87 "Net-(P2-Pad6)")
  (net 88 "Net-(P2-Pad7)")
  (net 89 "Net-(P2-Pad8)")
  (net 90 "Net-(P3-Pad1)")
  (net 91 "Net-(P3-Pad5)")
  (net 92 "Net-(P3-Pad7)")
  (net 93 "Net-(R4-Pad2)")
  (net 94 "Net-(R12-Pad2)")
  (net 95 "Net-(R15-Pad2)")
  (net 96 "Net-(R32-Pad2)")
  (net 97 "Net-(U1-Pad5)")
  (net 98 "Net-(U1-Pad30)")
  (net 99 "Net-(U1-Pad14)")
  (net 100 "Net-(U1-Pad15)")
  (net 101 "Net-(U2-Pad11)")
  (net 102 "Net-(U2-Pad12)")
  (net 103 "Net-(U2-Pad13)")
  (net 104 "Net-(U2-Pad14)")
  (net 105 "Net-(U2-Pad17)")
  (net 106 "Net-(U2-Pad18)")
  (net 107 "Net-(U2-Pad19)")
  (net 108 "Net-(U2-Pad20)")
  (net 109 "Net-(U4-Pad1)")
  (net 110 "Net-(U4-Pad5)")
  (net 111 "Net-(U5-Pad2)")
  (net 112 "Net-(U5-Pad6)")
  (net 113 "Net-(U5-Pad7)")
  (net 114 "Net-(U5-Pad8)")
  (net 115 "Net-(U5-Pad9)")
  (net 116 "Net-(U5-Pad10)")
  (net 117 "Net-(U5-Pad11)")
  (net 118 "Net-(U5-Pad14)")
  (net 119 "Net-(U5-Pad15)")
  (net 120 "Net-(U14-Pad3)")
  (net 121 "Net-(U14-Pad2)")
  (net 122 "Net-(U14-Pad4)")
  (net 123 "Net-(U5-Pad29)")
  (net 124 "Net-(U5-Pad33)")
  (net 125 "Net-(U5-Pad35)")
  (net 126 "Net-(U5-Pad67)")
  (net 127 "Net-(U5-Pad68)")
  (net 128 "Net-(U5-Pad69)")
  (net 129 "Net-(U5-Pad70)")
  (net 130 "Net-(U5-Pad72)")
  (net 131 "Net-(U5-Pad115)")
  (net 132 "Net-(U5-Pad116)")
  (net 133 "Net-(U5-Pad117)")
  (net 134 "Net-(U5-Pad120)")
  (net 135 "Net-(U5-Pad125)")
  (net 136 "Net-(U5-Pad126)")
  (net 137 "Net-(U5-Pad129)")
  (net 138 "Net-(U5-Pad130)")
  (net 139 "Net-(U5-Pad132)")
  (net 140 "Net-(U5-Pad133)")
  (net 141 "Net-(U5-Pad134)")
  (net 142 "Net-(U5-Pad136)")
  (net 143 "Net-(U5-Pad138)")
  (net 144 "Net-(U5-Pad139)")
  (net 145 "Net-(U5-Pad140)")
  (net 146 "Net-(U5-Pad142)")
  (net 147 "Net-(U5-Pad143)")
  (net 148 "Net-(U5-Pad144)")
  (net 149 "Net-(U5-Pad37)")
  (net 150 "Net-(U5-Pad38)")
  (net 151 "Net-(U5-Pad39)")
  (net 152 "Net-(U5-Pad44)")
  (net 153 "Net-(U5-Pad46)")
  (net 154 "Net-(U5-Pad47)")
  (net 155 "Net-(U5-Pad49)")
  (net 156 "Net-(U5-Pad54)")
  (net 157 "Net-(U5-Pad57)")
  (net 158 "Net-(U5-Pad58)")
  (net 159 "Net-(U5-Pad63)")
  (net 160 "Net-(U5-Pad65)")
  (net 161 "Net-(U5-Pad80)")
  (net 162 "Net-(U5-Pad82)")
  (net 163 "Net-(U5-Pad83)")
  (net 164 "Net-(U5-Pad85)")
  (net 165 "Net-(U5-Pad86)")
  (net 166 "Net-(U5-Pad87)")
  (net 167 "Net-(U5-Pad88)")
  (net 168 "Net-(U5-Pad89)")
  (net 169 "Net-(U5-Pad90)")
  (net 170 "Net-(U5-Pad91)")
  (net 171 "Net-(U5-Pad92)")
  (net 172 "Net-(U5-Pad93)")
  (net 173 "Net-(U5-Pad99)")
  (net 174 "Net-(U5-Pad103)")
  (net 175 "Net-(U5-Pad104)")
  (net 176 "Net-(U5-Pad105)")
  (net 177 "Net-(U5-Pad106)")
  (net 178 "Net-(U5-Pad108)")
  (net 179 "Net-(U5-Pad112)")
  (net 180 "Net-(U13-Pad1)")
  (net 181 "Net-(U13-Pad5)")
  (net 182 "Net-(C40-Pad1)")
  (net 183 "Net-(C42-Pad1)")
  (net 184 "Net-(C42-Pad2)")
  (net 185 "Net-(C43-Pad1)")
  (net 186 "Net-(C44-Pad1)")
  (net 187 "Net-(R25-Pad2)")
  (net 188 "Net-(U5-Pad53)")
  (net 189 "Net-(U5-Pad55)")
  (net 190 "Net-(U5-Pad56)")
  (net 191 "Net-(U5-Pad60)")
  (net 192 "Net-(U5-Pad61)")
  (net 193 "Net-(U5-Pad79)")
  (net 194 "Net-(U5-Pad73)")
  (net 195 "Net-(P4-Pad2)")
  (net 196 "Net-(P4-Pad3)")
  (net 197 "Net-(P4-Pad4)")
  (net 198 /TRIG_CONNECTED)
  (net 199 /TRIG_INT)
  (net 200 /TRIG_OUT)
  (net 201 "Net-(R31-Pad1)")
  (net 202 "Net-(R34-Pad1)")
  (net 203 "Net-(R39-Pad2)")
  (net 204 /TCAL_POWERED)
  (net 205 /TCAL_ATTACHED)
  (net 206 /TCAL_EN)
  (net 207 +3.3VADC)
  (net 208 "Net-(D7-Pad1)")
  (net 209 "Net-(D7-Pad2)")
  (net 210 "Net-(D8-Pad1)")
  (net 211 "Net-(D8-Pad2)")
  (net 212 "Net-(D9-Pad2)")
  (net 213 "Net-(D10-Pad1)")
  (net 214 "Net-(D11-Pad2)")
  (net 215 +3V3)
  (net 216 "Net-(U5-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.175)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.2)
    (uvia_drill 0.127)
    (add_net +12V)
    (add_net +3.3VADC)
    (add_net +3V3)
    (add_net +5V)
    (add_net /TCAL_ATTACHED)
    (add_net /TCAL_EN)
    (add_net /TCAL_POWERED)
    (add_net /TRIG_CONNECTED)
    (add_net /TRIG_INT)
    (add_net /TRIG_OUT)
    (add_net ADC_CLOCK)
    (add_net ATT1_SWITCH_A)
    (add_net ATT1_SWITCH_B)
    (add_net CP_OUT)
    (add_net GND)
    (add_net IF_AFTER_AMP1)
    (add_net IF_AFTER_AMP2)
    (add_net IF_AFTER_ATT1)
    (add_net IF_AFTER_FILTER)
    (add_net IF_AFTER_PREAMP)
    (add_net IF_AFTER_SAW)
    (add_net IF_FILTERED)
    (add_net IF_RAW)
    (add_net LO_CLOCK)
    (add_net LO_LOCK_DETECT)
    (add_net LO_RAW)
    (add_net LO_SPI_CLOCK)
    (add_net LO_SPI_DATA)
    (add_net LO_SPI_LE)
    (add_net "Net-(B1-Pad3)")
    (add_net "Net-(B1-Pad4)")
    (add_net "Net-(B1-Pad6)")
    (add_net "Net-(B2-Pad1)")
    (add_net "Net-(B2-Pad3)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C34-Pad1)")
    (add_net "Net-(C34-Pad2)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C38-Pad2)")
    (add_net "Net-(C39-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C40-Pad1)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C42-Pad1)")
    (add_net "Net-(C42-Pad2)")
    (add_net "Net-(C43-Pad1)")
    (add_net "Net-(C44-Pad1)")
    (add_net "Net-(C45-Pad1)")
    (add_net "Net-(C47-Pad2)")
    (add_net "Net-(C48-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C50-Pad1)")
    (add_net "Net-(C51-Pad1)")
    (add_net "Net-(C51-Pad2)")
    (add_net "Net-(C52-Pad1)")
    (add_net "Net-(C53-Pad1)")
    (add_net "Net-(C53-Pad2)")
    (add_net "Net-(C54-Pad1)")
    (add_net "Net-(C54-Pad2)")
    (add_net "Net-(C55-Pad1)")
    (add_net "Net-(C56-Pad2)")
    (add_net "Net-(C58-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(C61-Pad2)")
    (add_net "Net-(C62-Pad1)")
    (add_net "Net-(C78-Pad2)")
    (add_net "Net-(C79-Pad2)")
    (add_net "Net-(C80-Pad2)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(FB2-Pad2)")
    (add_net "Net-(L6-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R31-Pad1)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R34-Pad1)")
    (add_net "Net-(R39-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U13-Pad1)")
    (add_net "Net-(U13-Pad5)")
    (add_net "Net-(U14-Pad2)")
    (add_net "Net-(U14-Pad3)")
    (add_net "Net-(U14-Pad4)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad103)")
    (add_net "Net-(U5-Pad104)")
    (add_net "Net-(U5-Pad105)")
    (add_net "Net-(U5-Pad106)")
    (add_net "Net-(U5-Pad108)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad112)")
    (add_net "Net-(U5-Pad115)")
    (add_net "Net-(U5-Pad116)")
    (add_net "Net-(U5-Pad117)")
    (add_net "Net-(U5-Pad120)")
    (add_net "Net-(U5-Pad125)")
    (add_net "Net-(U5-Pad126)")
    (add_net "Net-(U5-Pad129)")
    (add_net "Net-(U5-Pad130)")
    (add_net "Net-(U5-Pad132)")
    (add_net "Net-(U5-Pad133)")
    (add_net "Net-(U5-Pad134)")
    (add_net "Net-(U5-Pad136)")
    (add_net "Net-(U5-Pad138)")
    (add_net "Net-(U5-Pad139)")
    (add_net "Net-(U5-Pad14)")
    (add_net "Net-(U5-Pad140)")
    (add_net "Net-(U5-Pad142)")
    (add_net "Net-(U5-Pad143)")
    (add_net "Net-(U5-Pad144)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad29)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U5-Pad33)")
    (add_net "Net-(U5-Pad35)")
    (add_net "Net-(U5-Pad37)")
    (add_net "Net-(U5-Pad38)")
    (add_net "Net-(U5-Pad39)")
    (add_net "Net-(U5-Pad44)")
    (add_net "Net-(U5-Pad46)")
    (add_net "Net-(U5-Pad47)")
    (add_net "Net-(U5-Pad49)")
    (add_net "Net-(U5-Pad53)")
    (add_net "Net-(U5-Pad54)")
    (add_net "Net-(U5-Pad55)")
    (add_net "Net-(U5-Pad56)")
    (add_net "Net-(U5-Pad57)")
    (add_net "Net-(U5-Pad58)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad60)")
    (add_net "Net-(U5-Pad61)")
    (add_net "Net-(U5-Pad63)")
    (add_net "Net-(U5-Pad65)")
    (add_net "Net-(U5-Pad67)")
    (add_net "Net-(U5-Pad68)")
    (add_net "Net-(U5-Pad69)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad70)")
    (add_net "Net-(U5-Pad72)")
    (add_net "Net-(U5-Pad73)")
    (add_net "Net-(U5-Pad79)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U5-Pad80)")
    (add_net "Net-(U5-Pad82)")
    (add_net "Net-(U5-Pad83)")
    (add_net "Net-(U5-Pad85)")
    (add_net "Net-(U5-Pad86)")
    (add_net "Net-(U5-Pad87)")
    (add_net "Net-(U5-Pad88)")
    (add_net "Net-(U5-Pad89)")
    (add_net "Net-(U5-Pad9)")
    (add_net "Net-(U5-Pad90)")
    (add_net "Net-(U5-Pad91)")
    (add_net "Net-(U5-Pad92)")
    (add_net "Net-(U5-Pad93)")
    (add_net "Net-(U5-Pad99)")
    (add_net RST)
    (add_net SKY)
    (add_net USB_BOOT)
    (add_net VCC)
    (add_net V_TUNE)
  )
  (module mycomponents:TQFP144 (layer F.Cu) (tedit 200000)
    (at 254 137.5 45)
    (attr smd)
    (fp_text reference U5 (at 0 -1.905 45) (layer F.SilkS))
    (fp_text value LPC4330FBD144 (at 0 1.905 45) (layer F.SilkS))
    (pad 1 smd rect (at 8.7503 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 8.2423 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U5-Pad2)"))
    (pad 3 smd rect (at 7.747 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(U5-Pad3)"))
    (pad 4 smd rect (at 7.2517 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at 6.7437 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 6 smd rect (at 6.2484 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U5-Pad6)"))
    (pad 7 smd rect (at 5.7531 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(U5-Pad7)"))
    (pad 8 smd rect (at 5.2451 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(U5-Pad8)"))
    (pad 9 smd rect (at 4.7498 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(U5-Pad9)"))
    (pad 10 smd rect (at 4.2545 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(U5-Pad10)"))
    (pad 11 smd rect (at 3.7465 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(U5-Pad11)"))
    (pad 12 smd rect (at 3.2512 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C38-Pad2)"))
    (pad 13 smd rect (at 2.7559 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C39-Pad2)"))
    (pad 14 smd rect (at 2.2479 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(U5-Pad14)"))
    (pad 15 smd rect (at 1.7526 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(U5-Pad15)"))
    (pad 16 smd rect (at 1.2573 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 17 smd rect (at 0.7493 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 18 smd rect (at 0.254 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(U14-Pad3)"))
    (pad 19 smd rect (at -0.254 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 20 smd rect (at -0.7493 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(U14-Pad2)"))
    (pad 21 smd rect (at -1.2573 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 25 VCC))
    (pad 22 smd rect (at -1.7526 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(U14-Pad4)"))
    (pad 23 smd rect (at -2.2479 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 24 smd rect (at -2.7559 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(R25-Pad2)"))
    (pad 25 smd rect (at -3.2512 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 26 smd rect (at -3.7465 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(P2-Pad8)"))
    (pad 27 smd rect (at -4.2545 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(P2-Pad4)"))
    (pad 28 smd rect (at -4.7498 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(R15-Pad2)"))
    (pad 29 smd rect (at -5.2451 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(U5-Pad29)"))
    (pad 30 smd rect (at -5.7531 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(P2-Pad2)"))
    (pad 31 smd rect (at -6.2484 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(P2-Pad6)"))
    (pad 32 smd rect (at -6.7437 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(U2-Pad20)"))
    (pad 33 smd rect (at -7.2517 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(U5-Pad33)"))
    (pad 34 smd rect (at -7.747 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-Pad19)"))
    (pad 35 smd rect (at -8.2423 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U5-Pad35)"))
    (pad 36 smd rect (at -8.7503 -10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 66 smd rect (at -10.9855 5.7531 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 3 ADC_CLOCK))
    (pad 67 smd rect (at -10.9855 6.2484 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U5-Pad67)"))
    (pad 68 smd rect (at -10.9855 6.7437 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(U5-Pad68)"))
    (pad 69 smd rect (at -10.9855 7.2517 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U5-Pad69)"))
    (pad 70 smd rect (at -10.9855 7.747 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(U5-Pad70)"))
    (pad 71 smd rect (at -10.9855 8.2423 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 72 smd rect (at -10.9855 8.7503 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(U5-Pad72)"))
    (pad 114 smd rect (at 10.9855 6.2484 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 17 LO_LOCK_DETECT))
    (pad 115 smd rect (at 10.9855 5.7531 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(U5-Pad115)"))
    (pad 116 smd rect (at 10.9855 5.2451 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(U5-Pad116)"))
    (pad 117 smd rect (at 10.9855 4.7498 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(U5-Pad117)"))
    (pad 118 smd rect (at 10.9855 4.2545 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 19 LO_SPI_CLOCK))
    (pad 119 smd rect (at 10.9855 3.7465 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(D5-Pad1)"))
    (pad 120 smd rect (at 10.9855 3.2512 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(U5-Pad120)"))
    (pad 121 smd rect (at 10.9855 2.7559 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 21 LO_SPI_LE))
    (pad 122 smd rect (at 10.9855 2.2479 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(D6-Pad1)"))
    (pad 123 smd rect (at 10.9855 1.7526 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 20 LO_SPI_DATA))
    (pad 124 smd rect (at 10.9855 1.2573 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D7-Pad1)"))
    (pad 125 smd rect (at 10.9855 0.7493 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(U5-Pad125)"))
    (pad 126 smd rect (at 10.9855 0.254 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(U5-Pad126)"))
    (pad 127 smd rect (at 10.9855 -0.254 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 128 smd rect (at 10.9855 -0.7493 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 22 RST))
    (pad 129 smd rect (at 10.9855 -1.2573 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(U5-Pad129)"))
    (pad 130 smd rect (at 10.9855 -1.7526 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(U5-Pad130)"))
    (pad 131 smd rect (at 10.9855 -2.2479 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 132 smd rect (at 10.9855 -2.7559 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(U5-Pad132)"))
    (pad 133 smd rect (at 10.9855 -3.2512 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(U5-Pad133)"))
    (pad 134 smd rect (at 10.9855 -3.7465 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(U5-Pad134)"))
    (pad 135 smd rect (at 10.9855 -4.2545 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 136 smd rect (at 10.9855 -4.7498 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(U5-Pad136)"))
    (pad 137 smd rect (at 10.9855 -5.2451 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 138 smd rect (at 10.9855 -5.7531 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(U5-Pad138)"))
    (pad 139 smd rect (at 10.9855 -6.2484 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U5-Pad139)"))
    (pad 140 smd rect (at 10.9855 -6.7437 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U5-Pad140)"))
    (pad 141 smd rect (at 10.9855 -7.2517 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 142 smd rect (at 10.9855 -7.747 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U5-Pad142)"))
    (pad 143 smd rect (at 10.9855 -8.2423 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U5-Pad143)"))
    (pad 144 smd rect (at 10.9855 -8.7503 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U5-Pad144)"))
    (pad 37 smd rect (at -10.9855 -8.7503 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U5-Pad37)"))
    (pad 38 smd rect (at -10.9855 -8.2423 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U5-Pad38)"))
    (pad 39 smd rect (at -10.9855 -7.747 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(U5-Pad39)"))
    (pad 40 smd rect (at -10.9855 -7.2517 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 41 smd rect (at -10.9855 -6.7437 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 42 smd rect (at -10.9855 -6.2484 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 24 USB_BOOT))
    (pad 43 smd rect (at -10.9855 -5.7531 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 44 smd rect (at -10.9855 -5.2451 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(U5-Pad44)"))
    (pad 45 smd rect (at -10.9855 -4.7498 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 3 ADC_CLOCK))
    (pad 46 smd rect (at -10.9855 -4.2545 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(U5-Pad46)"))
    (pad 47 smd rect (at -10.9855 -3.7465 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(U5-Pad47)"))
    (pad 48 smd rect (at -10.9855 -3.2512 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 3 ADC_CLOCK))
    (pad 49 smd rect (at -10.9855 -2.7559 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(U5-Pad49)"))
    (pad 50 smd rect (at -10.9855 -2.2479 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 204 /TCAL_POWERED))
    (pad 51 smd rect (at -10.9855 -1.7526 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 205 /TCAL_ATTACHED))
    (pad 52 smd rect (at -10.9855 -1.2573 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 206 /TCAL_EN))
    (pad 53 smd rect (at -10.9855 -0.7493 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(U5-Pad53)"))
    (pad 54 smd rect (at -10.9855 -0.254 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(U5-Pad54)"))
    (pad 55 smd rect (at -10.9855 0.254 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(U5-Pad55)"))
    (pad 56 smd rect (at -10.9855 0.7493 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(U5-Pad56)"))
    (pad 57 smd rect (at -10.9855 1.2573 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(U5-Pad57)"))
    (pad 58 smd rect (at -10.9855 1.7526 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(U5-Pad58)"))
    (pad 59 smd rect (at -10.9855 2.2479 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 60 smd rect (at -10.9855 2.7559 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(U5-Pad60)"))
    (pad 61 smd rect (at -10.9855 3.2512 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(U5-Pad61)"))
    (pad 62 smd rect (at -10.9855 3.7465 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U2-Pad18)"))
    (pad 63 smd rect (at -10.9855 4.2545 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(U5-Pad63)"))
    (pad 64 smd rect (at -10.9855 4.7498 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U2-Pad17)"))
    (pad 65 smd rect (at -10.9855 5.2451 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(U5-Pad65)"))
    (pad 78 smd rect (at -6.2484 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 ATT1_SWITCH_B))
    (pad 79 smd rect (at -5.7531 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(U5-Pad79)"))
    (pad 80 smd rect (at -5.2451 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(U5-Pad80)"))
    (pad 81 smd rect (at -4.7498 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(P3-Pad5)"))
    (pad 82 smd rect (at -4.2545 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U5-Pad82)"))
    (pad 83 smd rect (at -3.7465 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U5-Pad83)"))
    (pad 84 smd rect (at -3.2512 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U2-Pad12)"))
    (pad 85 smd rect (at -2.7559 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(U5-Pad85)"))
    (pad 86 smd rect (at -2.2479 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U5-Pad86)"))
    (pad 87 smd rect (at -1.7526 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U5-Pad87)"))
    (pad 88 smd rect (at -1.2573 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U5-Pad88)"))
    (pad 89 smd rect (at -0.7493 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(U5-Pad89)"))
    (pad 90 smd rect (at -0.254 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(U5-Pad90)"))
    (pad 91 smd rect (at 0.254 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(U5-Pad91)"))
    (pad 92 smd rect (at 0.7493 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(U5-Pad92)"))
    (pad 93 smd rect (at 1.2573 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(U5-Pad93)"))
    (pad 94 smd rect (at 1.7526 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 95 smd rect (at 2.2479 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U2-Pad11)"))
    (pad 96 smd rect (at 2.7559 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(P3-Pad1)"))
    (pad 97 smd rect (at 3.2512 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 199 /TRIG_INT))
    (pad 98 smd rect (at 3.7465 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 24 USB_BOOT))
    (pad 99 smd rect (at 4.2545 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(U5-Pad99)"))
    (pad 100 smd rect (at 4.7498 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 200 /TRIG_OUT))
    (pad 101 smd rect (at 5.2451 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 198 /TRIG_CONNECTED))
    (pad 102 smd rect (at 5.7531 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 103 smd rect (at 6.2484 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U5-Pad103)"))
    (pad 104 smd rect (at 6.7437 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U5-Pad104)"))
    (pad 105 smd rect (at 7.2517 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U5-Pad105)"))
    (pad 106 smd rect (at 7.747 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U5-Pad106)"))
    (pad 107 smd rect (at 8.2423 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 108 smd rect (at 8.7503 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U5-Pad108)"))
    (pad 73 smd rect (at -8.7503 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(U5-Pad73)"))
    (pad 74 smd rect (at -8.2423 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 ATT1_SWITCH_A))
    (pad 75 smd rect (at -7.747 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(P3-Pad7)"))
    (pad 76 smd rect (at -7.2517 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 77 smd rect (at -6.7437 10.9855 45) (size 0.254 1.524) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 109 smd rect (at 10.9855 8.7503 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 110 smd rect (at 10.9855 8.2423 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(U2-Pad14)"))
    (pad 111 smd rect (at 10.9855 7.747 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 112 smd rect (at 10.9855 7.2517 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U5-Pad112)"))
    (pad 113 smd rect (at 10.9855 6.7437 45) (size 1.524 0.254) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(U2-Pad13)"))
    (model smd/tqfp144.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SSOP20_AD9283 (layer F.Cu) (tedit 55159A80)
    (at 230.251 126.746 270)
    (descr "SSOP 20 pins")
    (tags "CMS SSOP SMD")
    (attr smd)
    (fp_text reference U2 (at 4.454 -0.8 360) (layer F.SilkS))
    (fp_text value AD9283 (at 0 0.635 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.921 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -2.286 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (pad 3 smd rect (at -1.6256 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (pad 4 smd rect (at -0.9652 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at -0.3302 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 6 smd rect (at 0.3302 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C3-Pad1)"))
    (pad 7 smd rect (at 0.9906 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 13 IF_AFTER_SAW))
    (pad 8 smd rect (at 1.6256 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 9 smd rect (at 2.286 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 10 smd rect (at 2.921 4.5 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 ADC_CLOCK))
    (pad 11 smd rect (at 2.921 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 2.286 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 1.6256 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 0.9906 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 0.3302 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 16 smd rect (at -0.3302 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 17 smd rect (at -0.9652 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at -1.6256 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U2-Pad18)"))
    (pad 19 smd rect (at -2.286 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at -2.921 -3.275 270) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(U2-Pad20)"))
    (model smd/cms_so20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.255 0.33 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:QUARTZ_AVX_PBRC (layer F.Cu) (tedit 55155686)
    (at 261 118.872 180)
    (fp_text reference X2 (at -4.6 1.172 180) (layer F.SilkS))
    (fp_text value CRYSTAL_SMD (at 0 -2.8 180) (layer F.SilkS))
    (pad 3 smd rect (at 0 0 180) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -2.5 0 180) (size 1.7 4) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C39-Pad2)"))
    (pad 2 smd rect (at 2.5 0 180) (size 1.7 4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C38-Pad2)"))
    (model lib/avx_ceramic_resonator.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.91 2.91 2.91))
      (rotate (xyz 270 0 90))
    )
  )
  (module mycomponents:PC357NJ0000F (layer B.Cu) (tedit 54E0C9C1)
    (at 254.381 156.591)
    (fp_text reference U12 (at 3.937 -2.286) (layer B.SilkS))
    (fp_text value OPTO-TRANSISTOR4 (at 0 4.445) (layer B.Fab))
    (pad 1 smd rect (at -3.15 1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -3.15 -1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 202 "Net-(R34-Pad1)"))
    (pad 3 smd rect (at 3.15 -1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 205 /TCAL_ATTACHED))
    (pad 4 smd rect (at 3.15 1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 207 +3.3VADC))
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F36B)
    (at 228.35042 131.6)
    (attr smd)
    (fp_text reference C89 (at 0.64958 1.1) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0DA78)
    (at 181.9 144.8)
    (attr smd)
    (fp_text reference L6 (at 1.996 -0.02 180) (layer F.SilkS))
    (fp_text value 6.8nH (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(L6-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer B.Cu) (tedit 542FB43A)
    (at 235.966 142.24)
    (attr smd)
    (fp_text reference R28 (at 0 -1.397) (layer B.SilkS))
    (fp_text value 4k7 (at -1.69926 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 195 "Net-(P4-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer B.Cu) (tedit 551AD563)
    (at 236.474 151.765 270)
    (attr smd)
    (fp_text reference R31 (at 0.135 1.374 270) (layer B.SilkS))
    (fp_text value R (at -1.69926 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 201 "Net-(R31-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 197 "Net-(P4-Pad4)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer B.Cu) (tedit 542FB43A)
    (at 253.238 152.908 180)
    (attr smd)
    (fp_text reference R34 (at -0.127 1.143 180) (layer B.SilkS))
    (fp_text value R (at -1.69926 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 202 "Net-(R34-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 196 "Net-(P4-Pad3)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer B.Cu) (tedit 542FB43A)
    (at 232.156 142.24 180)
    (attr smd)
    (fp_text reference R39 (at 0 1.397 180) (layer B.SilkS))
    (fp_text value R (at -1.69926 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 203 "Net-(R39-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 542FB43A)
    (at 243.078 148.082 90)
    (attr smd)
    (fp_text reference R40 (at 0 1.397 270) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 204 /TCAL_POWERED))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer B.Cu) (tedit 551AD55E)
    (at 232.537 152.273 180)
    (attr smd)
    (fp_text reference R46 (at 0.037 1.473 180) (layer B.SilkS))
    (fp_text value 4k7 (at -1.69926 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 205 /TCAL_ATTACHED))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer B.Cu) (tedit 551AD54F)
    (at 238.125 151.765 90)
    (attr smd)
    (fp_text reference R47 (at -0.035 1.575 90) (layer B.SilkS))
    (fp_text value 4k7 (at -1.69926 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 198 /TRIG_CONNECTED))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:PC357NJ0000F (layer B.Cu) (tedit 551AD55B)
    (at 234.569 145.923)
    (fp_text reference U6 (at 3.531 -2.523) (layer B.SilkS))
    (fp_text value OPTO-TRANSISTOR4 (at 0 4.445) (layer B.Fab))
    (pad 1 smd rect (at -3.15 1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 206 /TCAL_EN))
    (pad 2 smd rect (at -3.15 -1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 203 "Net-(R39-Pad2)"))
    (pad 3 smd rect (at 3.15 -1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 195 "Net-(P4-Pad2)"))
    (pad 4 smd rect (at 3.15 1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
  )
  (module mycomponents:PC357NJ0000F (layer B.Cu) (tedit 551AD555)
    (at 243.967 150.749)
    (fp_text reference U8 (at -1.767 -3.249) (layer B.SilkS))
    (fp_text value OPTO-TRANSISTOR4 (at 0 4.445) (layer B.Fab))
    (pad 1 smd rect (at -3.15 1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 201 "Net-(R31-Pad1)"))
    (pad 2 smd rect (at -3.15 -1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 3.15 -1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 204 /TCAL_POWERED))
    (pad 4 smd rect (at 3.15 1.27) (size 1.5 0.8) (layers B.Cu B.Paste B.Mask)
      (net 207 +3.3VADC))
  )
  (module mycomponents:HM1522B1 (layer F.Cu) (tedit 541DCF5B)
    (at 182.3 151.8 90)
    (fp_text reference B1 (at 0 0 90) (layer F.SilkS))
    (fp_text value HM1522 (at 0 -1.4 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.65 -0.65 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 SKY) (clearance 0.1))
    (pad 2 smd rect (at 0 -0.65 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 3 smd rect (at 0.65 -0.65 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(B1-Pad3)") (clearance 0.1))
    (pad 4 smd rect (at 0.65 0.65 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(B1-Pad4)") (clearance 0.1))
    (pad 5 smd rect (at 0 0.65 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 6 smd rect (at -0.65 0.65 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(B1-Pad6)") (clearance 0.1))
    (model lib/HHM1515B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.787 0.787 0.787))
      (rotate (xyz 270 0 90))
    )
  )
  (module mycomponents:MABAES0061 (layer F.Cu) (tedit 551AD2D8)
    (at 194.7 148.8 90)
    (fp_text reference B2 (at -2.7 1.6 180) (layer F.SilkS))
    (fp_text value MABAES0061 (at 0 -0.3 90) (layer F.SilkS))
    (pad 5 smd rect (at -1.27 1.715 90) (size 0.76 1.4) (layers F.Cu F.Paste F.Mask)
      (net 15 IF_RAW) (clearance 0.1))
    (pad 4 smd rect (at 1.27 1.715 90) (size 0.76 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 1 smd rect (at 1.27 -1.715 90) (size 0.76 1.4) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(B2-Pad1)") (clearance 0.1))
    (pad 2 smd rect (at 0 -1.715 90) (size 0.76 1.4) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3) (clearance 0.1))
    (pad 3 smd rect (at -1.27 -1.715 90) (size 0.76 1.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(B2-Pad3)") (clearance 0.1))
    (model lib/MABAES0029.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.1 2.1 2.1))
      (rotate (xyz 270 0 -90))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0DA8E)
    (at 182.3 153.7)
    (attr smd)
    (fp_text reference C1 (at 2.104 -0.03 180) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 SKY))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C1-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D7B3)
    (at 210.8 136.4)
    (attr smd)
    (fp_text reference C2 (at -2.139 -0.002 180) (layer F.SilkS))
    (fp_text value 39pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 IF_AFTER_AMP1))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 55159B92)
    (at 224 127.1 180)
    (attr smd)
    (fp_text reference C3 (at 1.2 0.2 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C3-Pad2)"))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D7AF)
    (at 210.8 133.25 180)
    (attr smd)
    (fp_text reference C4 (at 2.012 -0.1 360) (layer F.SilkS))
    (fp_text value 20pF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 IF_AFTER_AMP1))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 55159B97)
    (at 224.3 123.54958 90)
    (attr smd)
    (fp_text reference C5 (at 0.64958 1.4 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D67B)
    (at 185 138.6)
    (attr smd)
    (fp_text reference C6 (at -2.12 0.084 180) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 LO_RAW))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C6-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 55159B83)
    (at 224 126)
    (attr smd)
    (fp_text reference C7 (at 0.1 -1) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D7AA)
    (at 213.8 134.85 180)
    (attr smd)
    (fp_text reference C8 (at -2.1 -0.024 360) (layer F.SilkS))
    (fp_text value 39pF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 IF_AFTER_FILTER))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0DA7E)
    (at 182.3 150)
    (attr smd)
    (fp_text reference C9 (at -1.325 -1.41 180) (layer F.SilkS))
    (fp_text value 2.2pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(B1-Pad3)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(B1-Pad4)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0DA76)
    (at 180.35 143.3)
    (attr smd)
    (fp_text reference C10 (at 2.403 -0.044 180) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 LO_RAW))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C10-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D6DF)
    (at 188.4 127.4 90)
    (attr smd)
    (fp_text reference C11 (at 2.559 2.862 90) (layer F.SilkS))
    (fp_text value 10pF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D6DC)
    (at 189.3 127.4 90)
    (attr smd)
    (fp_text reference C12 (at 2.559 3.105 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D70C)
    (at 189.8 128.6)
    (attr smd)
    (fp_text reference C13 (at 3.113 -1.473) (layer F.SilkS))
    (fp_text value 10pF (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D70F)
    (at 189.8 129.5)
    (attr smd)
    (fp_text reference C14 (at 3.113 -1.357) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.44958 0) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D663)
    (at 189.4 135.8 270)
    (attr smd)
    (fp_text reference C15 (at 3.519 -3.767 270) (layer F.SilkS))
    (fp_text value 10pF (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D66D)
    (at 188.5 135.8 270)
    (attr smd)
    (fp_text reference C16 (at 3.519 -3.524 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0DA74)
    (at 185.8 144.5 90)
    (attr smd)
    (fp_text reference C17 (at 1.371 1.906 180) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0DA81)
    (at 187.2 148.8 270)
    (attr smd)
    (fp_text reference C18 (at 2.584 0.002 450) (layer F.SilkS))
    (fp_text value 1.5pF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C18-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D680)
    (at 183.75 135.3 180)
    (attr smd)
    (fp_text reference C19 (at 2.775 -0.082 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D6FB)
    (at 184.7 126.2)
    (attr smd)
    (fp_text reference C20 (at 0.466 1.308 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 LO_CLOCK))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D6AB)
    (at 180.9 132.5 180)
    (attr smd)
    (fp_text reference C21 (at 0.687 -1.358 360) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 CP_OUT))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D675)
    (at 187.6 135.8 270)
    (attr smd)
    (fp_text reference C22 (at 3.519 -3.281 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0DA6F)
    (at 187.1 146.2 90)
    (attr smd)
    (fp_text reference C23 (at 1.928 2.892 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D651)
    (at 193.6 133.7 90)
    (attr smd)
    (fp_text reference C24 (at -2.571 0.202 270) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D6A7)
    (at 182.3 131.3 180)
    (attr smd)
    (fp_text reference C25 (at -0.453 -1.669 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0DA6C)
    (at 188 146.2 90)
    (attr smd)
    (fp_text reference C26 (at 1.928 3.135 90) (layer F.SilkS))
    (fp_text value 100pF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D6F7)
    (at 183.2 127.6 180)
    (attr smd)
    (fp_text reference C27 (at 0.955 1.108 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 180) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 180) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 551AD26A)
    (at 184.7 123.2 180)
    (attr smd)
    (fp_text reference C28 (at 0 1.4 360) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C28-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C20-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D704)
    (at 187.5 126.5 90)
    (attr smd)
    (fp_text reference C29 (at 3.945 0.46 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0DAC7)
    (at 190.6 133.7 270)
    (attr smd)
    (fp_text reference C30 (at 3.587 -1.297 540) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 V_TUNE))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D702)
    (at 186.4 126.2 90)
    (attr smd)
    (fp_text reference C31 (at 3.645 0.417 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D7B9)
    (at 212.8 139.8)
    (attr smd)
    (fp_text reference C32 (at -2.488 0.027 180) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 IF_AFTER_FILTER))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 55117C76)
    (at 202.5 149.3 90)
    (attr smd)
    (fp_text reference C33 (at 2.9 1.4 270) (layer F.SilkS))
    (fp_text value 12pF (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 IF_RAW))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D7D2)
    (at 217.7 147.6 90)
    (attr smd)
    (fp_text reference C34 (at 0.026 1.375 270) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C34-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D7C9)
    (at 217.7 144.7 90)
    (attr smd)
    (fp_text reference C35 (at 2.206 0.994 180) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 55117C7E)
    (at 200.3 149.3 270)
    (attr smd)
    (fp_text reference C36 (at -0.1 1.3 450) (layer F.SilkS))
    (fp_text value 24pF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C36-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 IF_RAW))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 55117C73)
    (at 202.5 146.4 270)
    (attr smd)
    (fp_text reference C37 (at 2.9 -1.4 450) (layer F.SilkS))
    (fp_text value 18pF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 IF_FILTERED))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E4F433)
    (at 259.762 115.824 180)
    (attr smd)
    (fp_text reference C38 (at 2.462 -0.076 360) (layer F.SilkS))
    (fp_text value 39pF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C38-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E4F436)
    (at 262.5 115.824)
    (attr smd)
    (fp_text reference C39 (at 2.5 0.076 180) (layer F.SilkS))
    (fp_text value 39pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C39-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 55159B8B)
    (at 221.6 127 90)
    (attr smd)
    (fp_text reference C40 (at -1.1 2 180) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(C40-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D745)
    (at 200.8 143.1)
    (attr smd)
    (fp_text reference C41 (at 2.4 -0.098 180) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C41-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 IF_FILTERED))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D65E)
    (at 187.5028 138.8872 180)
    (attr smd)
    (fp_text reference C42 (at -1.9812 -0.4318 270) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(C42-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(C42-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 551AD3BA)
    (at 211.709 151.003)
    (attr smd)
    (fp_text reference C43 (at -2.509 -0.103 180) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(C43-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 542F3301)
    (at 216.2 123.1 180)
    (attr smd)
    (fp_text reference C44 (at 0.1 1.3 360) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(C44-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 551463F9)
    (at 198.2 136.6 180)
    (attr smd)
    (fp_text reference C45 (at 1.9 -0.05 450) (layer F.SilkS))
    (fp_text value 2.2uF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 551463F7)
    (at 198.2 135.1 180)
    (attr smd)
    (fp_text reference C46 (at -5.05 0 360) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 551463E5)
    (at 197.8 133.6)
    (attr smd)
    (fp_text reference C47 (at 5.25 0 180) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C47-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D742)
    (at 203.2 137.7 270)
    (attr smd)
    (fp_text reference C48 (at 2.889 -2.032 450) (layer F.SilkS))
    (fp_text value 100pF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 IF_AFTER_PREAMP))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C48-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 551463CA)
    (at 202.4 130.5)
    (attr smd)
    (fp_text reference C50 (at -2.9 0 180) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C50-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 IF_AFTER_PREAMP))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 542F3301)
    (at 203.2 125.3 180)
    (attr smd)
    (fp_text reference C51 (at -0.508 -1.827 270) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C51-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C51-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D7F0)
    (at 224.7652 145.9412)
    (attr smd)
    (fp_text reference C52 (at 1.4218 1.3788 180) (layer F.SilkS))
    (fp_text value 3.3pF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C52-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 542F3301)
    (at 200.1 124.5 270)
    (attr smd)
    (fp_text reference C53 (at -0.04 1.218 450) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C53-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C53-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 542F3301)
    (at 203.2 123.7)
    (attr smd)
    (fp_text reference C54 (at 0.508 -1.907 90) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C54-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C54-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 551469C9)
    (at 223.1152 137.6912 180)
    (attr smd)
    (fp_text reference C55 (at 0.1152 1.4912 360) (layer F.SilkS))
    (fp_text value 3.3pF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C55-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 55117CEB)
    (at 202.4 118.5 180)
    (attr smd)
    (fp_text reference C56 (at -2.4 0 360) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 IF_AFTER_ATT1))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C56-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D760)
    (at 210.55 118.1 90)
    (attr smd)
    (fp_text reference C58 (at 0.752 -1.254 270) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C58-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 IF_AFTER_ATT1))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D79D)
    (at 209.25 129.3)
    (attr smd)
    (fp_text reference C61 (at 6.65 -1.792 90) (layer F.SilkS))
    (fp_text value 1nF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C61-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C61-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E0D795)
    (at 212.9 129.2)
    (attr smd)
    (fp_text reference C62 (at 4.778 -1.692 90) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C62-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F461)
    (at 268.5 141 45)
    (attr smd)
    (fp_text reference C63 (at -0.443356 1.310269 45) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 45) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 45) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 45) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 542F32C1)
    (at 250 123.7 225)
    (attr smd)
    (fp_text reference C64 (at 2 0 225) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 225) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 542F32C1)
    (at 245.4 126 225)
    (attr smd)
    (fp_text reference C65 (at 2 0 225) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 225) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F44B)
    (at 261.6 127.3 135)
    (attr smd)
    (fp_text reference C66 (at -0.071418 1.214102 135) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 135) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 135) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 135) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 542F32C1)
    (at 246.5 127.1 225)
    (attr smd)
    (fp_text reference C67 (at 2 0 225) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 225) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F446)
    (at 257.4 123.1 315)
    (attr smd)
    (fp_text reference C68 (at -0.095459 -1.214102 315) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 315) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 315) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 315) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F459)
    (at 268.8 134.4 135)
    (attr smd)
    (fp_text reference C69 (at 1.957979 0.604576 135) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 135) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 135) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 135) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F44D)
    (at 258.8 124.5 315)
    (attr smd)
    (fp_text reference C70 (at 0.349311 -1.1243 315) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 315) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 315) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 315) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F472)
    (at 257.9 151.4 45)
    (attr smd)
    (fp_text reference C71 (at 0.755897 1.272085 45) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 45) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 45) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 45) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F47D)
    (at 246.2 147.9 45)
    (attr smd)
    (fp_text reference C72 (at -0.450427 1.064196 45) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 45) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 45) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 45) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4CC85)
    (at 243.1 130.5 225)
    (attr smd)
    (fp_text reference C73 (at -0.393858 1.143392 225) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 225) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F452)
    (at 263.1 128.8 135)
    (attr smd)
    (fp_text reference C74 (at -0.374767 1.1243 135) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 135) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 135) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 135) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 542F32C1)
    (at 251.3 152.6 135)
    (attr smd)
    (fp_text reference C75 (at 2 0 135) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 135) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 135) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 135) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E4C869)
    (at 230.378 154.686 270)
    (attr smd)
    (fp_text reference C77 (at 2.54 -0.127 450) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D697)
    (at 180.9 127.4 270)
    (attr smd)
    (fp_text reference C78 (at -5.734 0.179 360) (layer F.SilkS))
    (fp_text value 1nF (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C78-Pad2)"))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D6C4)
    (at 180.9 129 270)
    (attr smd)
    (fp_text reference C79 (at -6.318 0.179 360) (layer F.SilkS))
    (fp_text value 1nF (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C79-Pad2)"))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E0D69F)
    (at 180.9 130.7 90)
    (attr smd)
    (fp_text reference C80 (at 6.875 -0.179 180) (layer F.SilkS))
    (fp_text value 1nF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C80-Pad2)"))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E4C7F6)
    (at 212.09 154.686 270)
    (attr smd)
    (fp_text reference C81 (at 2.413 0 450) (layer F.SilkS))
    (fp_text value 2.2uF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Capa_s (layer F.Cu) (tedit 54E4C7F8)
    (at 213.868 154.686 270)
    (attr smd)
    (fp_text reference C82 (at 2.413 0 450) (layer F.SilkS))
    (fp_text value 100nF (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4F467)
    (at 264.6 144.9 225)
    (attr smd)
    (fp_text reference C83 (at -0.402344 -1.310269 225) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 225) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 225) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 54E4CC73)
    (at 238.6 135.2 45)
    (attr smd)
    (fp_text reference C84 (at -0.105359 -1.105208 45) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 45) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 45) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 45) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 542F32C1)
    (at 239.9 141.9 315)
    (attr smd)
    (fp_text reference C85 (at 2 0 315) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 315) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 315) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 315) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 542F32C1)
    (at 235.077 126.746 270)
    (attr smd)
    (fp_text reference C88 (at 2 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.44958 0 270) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0402_s (layer F.Cu) (tedit 55146E49)
    (at 193.2 119.6 90)
    (attr smd)
    (fp_text reference C90 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 100nF (at 0.09906 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.44958 0 90) (size 0.39878 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\chip_cms.wrl
      (at (xyz 0 0 0.002))
      (scale (xyz 0.05 0.05 0.05))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:LUMBERG_SMT_PLUG (layer F.Cu) (tedit 549965C5)
    (at 263.9 152)
    (fp_text reference CON1 (at 7.3 -1.7) (layer F.SilkS) hide)
    (fp_text value BARREL_JACK (at 2.6 -4) (layer F.SilkS))
    (pad 3 smd rect (at 11.1 -6.5) (size 2.7 2) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 5 -6.5) (size 2.7 2) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at 5 6.5) (size 2.7 2) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(CON1-Pad1)"))
    (pad 1 smd rect (at 11.1 6.5) (size 2.7 2) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(CON1-Pad1)"))
    (pad 4 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 9.5 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask F.SilkS))
  )
  (module mycomponents:DIODE_B0530W (layer F.Cu) (tedit 551A92E4)
    (at 263 158.5 180)
    (fp_text reference D1 (at -0.2 -2.6 180) (layer F.SilkS) hide)
    (fp_text value DIODE (at 0 -0.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.85 0 180) (size 1.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(CON1-Pad1)"))
    (pad 2 smd rect (at 1.85 0 180) (size 1.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 54E4CB6D)
    (at 274.7 130 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -3.81 -0.508 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D2-Pad2)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 54E4CB6F)
    (at 274.7 128.4 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -4.1 -3.8 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(D3-Pad2)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 55146E4D)
    (at 182.2 119.4 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0.8 1.6 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.016 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 17 LO_LOCK_DETECT))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(D4-Pad2)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 551A92D7)
    (at 274.5 118.2 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at -4.9 -0.291 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(D5-Pad2)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 551A92D9)
    (at 274.5 116 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at -4.392 -0.713 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(D6-Pad2)"))
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551463E3)
    (at 200.4 133.6)
    (attr smd)
    (fp_text reference FB1 (at 4.85 0 180) (layer F.SilkS))
    (fp_text value FILTER (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C47-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551AF9EB)
    (at 200.8 135.1)
    (attr smd)
    (fp_text reference FB2 (at 4.7 0 180) (layer F.SilkS))
    (fp_text value FILTER (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C47-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(FB2-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D76B)
    (at 214 126.6 90)
    (attr smd)
    (fp_text reference FB3 (at 2.394 0.122 270) (layer F.SilkS))
    (fp_text value FILTER (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C62-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D7AC)
    (at 213.8 133.25)
    (attr smd)
    (fp_text reference L2 (at 1.973 -0.027 180) (layer F.SilkS))
    (fp_text value 100nH (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 IF_AFTER_FILTER))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0DA8B)
    (at 185.1 151.7 270)
    (attr smd)
    (fp_text reference L4 (at 1.716 -1.463 360) (layer F.SilkS))
    (fp_text value 100nH (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(B1-Pad4)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0DA93)
    (at 179.5 151.7 270)
    (attr smd)
    (fp_text reference L5 (at -1.967 -0.078 450) (layer F.SilkS))
    (fp_text value 100nH (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(B1-Pad3)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0DA88)
    (at 189.2 148.1)
    (attr smd)
    (fp_text reference L7 (at 1.173 -1.288 180) (layer F.SilkS))
    (fp_text value 220nH (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(B2-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0DA85)
    (at 189.2 149.6)
    (attr smd)
    (fp_text reference L8 (at 1.046 1.276 180) (layer F.SilkS))
    (fp_text value 220nH (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C18-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(B2-Pad3)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 55117C7A)
    (at 200.3 146.4 90)
    (attr smd)
    (fp_text reference L10 (at 0.1 -1.3 270) (layer F.SilkS))
    (fp_text value 100nH (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C36-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 IF_FILTERED))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D740)
    (at 201.8 137.7 270)
    (attr smd)
    (fp_text reference L12 (at 2.889 -2.289 450) (layer F.SilkS))
    (fp_text value 820nH (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(FB2-Pad2)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C48-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D7ED)
    (at 222.7652 146.4412 90)
    (attr smd)
    (fp_text reference L13 (at 0.0102 -1.2772 270) (layer F.SilkS))
    (fp_text value 47nH (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 IF_AFTER_AMP2))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C52-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 55146A20)
    (at 225.2152 136.9912 90)
    (attr smd)
    (fp_text reference L14 (at 0.7912 1.3848 270) (layer F.SilkS))
    (fp_text value 56nH (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C55-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 IF_AFTER_SAW))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:micro_2x5_pin (layer F.Cu) (tedit 541D7355)
    (at 237.49 118.237)
    (fp_text reference P2 (at 0 -5.08) (layer F.SilkS))
    (fp_text value CONN_10 (at 0 -6.35) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at -1.27 -1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(P2-Pad2)"))
    (pad 3 smd rect (at 0 -1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 4 smd rect (at 1.27 -1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(P2-Pad4)"))
    (pad 5 smd rect (at 2.54 -1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 6 smd rect (at -2.54 1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(P2-Pad6)"))
    (pad 7 smd rect (at -1.27 1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(P2-Pad7)"))
    (pad 8 smd rect (at 0 1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(P2-Pad8)"))
    (pad 9 smd rect (at 1.27 1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 10 smd rect (at 2.54 1.905) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 RST))
    (model lib/2x5pin_127.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.75 2.75 2.75))
      (rotate (xyz 270 0 90))
    )
  )
  (module mycomponents:micro_2x5_pin (layer F.Cu) (tedit 551A92E1)
    (at 273 138.5 270)
    (fp_text reference P3 (at 0 -5.08 270) (layer F.SilkS) hide)
    (fp_text value CONN_10 (at 0 -6.35 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at -1.27 -1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 0 -1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 RST))
    (pad 4 smd rect (at 1.27 -1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at 2.54 -1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(P3-Pad5)"))
    (pad 6 smd rect (at -2.54 1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 7 smd rect (at -1.27 1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(P3-Pad7)"))
    (pad 8 smd rect (at 0 1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 9 smd rect (at 1.27 1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 24 USB_BOOT))
    (pad 10 smd rect (at 2.54 1.905 270) (size 0.42 2.5) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model lib/2x5pin_127.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.75 2.75 2.75))
      (rotate (xyz 270 0 90))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 55159B9C)
    (at 222.6 124.3 90)
    (attr smd)
    (fp_text reference R1 (at 0.2 -1.3 90) (layer F.SilkS))
    (fp_text value 25R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D67E)
    (at 185 137.1 180)
    (attr smd)
    (fp_text reference R2 (at 3.263 -0.06 360) (layer F.SilkS))
    (fp_text value 50 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D671)
    (at 187.5 137.4)
    (attr smd)
    (fp_text reference R3 (at 1.984 0.014 180) (layer F.SilkS))
    (fp_text value 50 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(C42-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551AD28C)
    (at 191.9 130.1 180)
    (attr smd)
    (fp_text reference R4 (at -2 0 450) (layer F.SilkS))
    (fp_text value 4k7 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(R4-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551AD268)
    (at 184.7 124.7)
    (attr smd)
    (fp_text reference R5 (at -1.8 -0.1 270) (layer F.SilkS))
    (fp_text value 50R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D64C)
    (at 192.1 133.7 270)
    (attr smd)
    (fp_text reference R6 (at 2.19 -0.559 450) (layer F.SilkS))
    (fp_text value 220 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 CP_OUT))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C24-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 542F33AC)
    (at 191.1 131.6)
    (attr smd)
    (fp_text reference R7 (at 2 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 V_TUNE))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 CP_OUT))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D7C4)
    (at 215.3 139.8)
    (attr smd)
    (fp_text reference R8 (at 1.997 0.027 180) (layer F.SilkS))
    (fp_text value 50R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 IF_AFTER_FILTER))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D7C6)
    (at 212.8 141.3 180)
    (attr smd)
    (fp_text reference R9 (at -2.338 -0.051 360) (layer F.SilkS))
    (fp_text value 2k2 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C32-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D7C2)
    (at 211.3 142.8 180)
    (attr smd)
    (fp_text reference R10 (at -2.441 0.052 360) (layer F.SilkS))
    (fp_text value 2k2 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E4F46E)
    (at 262 148.5 225)
    (attr smd)
    (fp_text reference R11 (at 0.565685 -1.838478 405) (layer F.SilkS))
    (fp_text value 4k7 (at 0 0 225) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 225) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 0.762 0 225) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551AD3BE)
    (at 211.7 149.5)
    (attr smd)
    (fp_text reference R12 (at -2.4 0 180) (layer F.SilkS))
    (fp_text value 9R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(C43-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(R12-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551AD3B6)
    (at 214.2 149.5 180)
    (attr smd)
    (fp_text reference R13 (at -1.5 -1.4 360) (layer F.SilkS))
    (fp_text value 174R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C34-Pad2)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(R12-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D7CD)
    (at 217.7 150.1 90)
    (attr smd)
    (fp_text reference R14 (at -0.014 1.375 90) (layer F.SilkS))
    (fp_text value 1R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 IF_AFTER_AMP2))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C34-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 551176CE)
    (at 238.887 123.825 315)
    (attr smd)
    (fp_text reference R15 (at 0 1.436841 495) (layer F.SilkS))
    (fp_text value 0R (at -1.69926 0 405) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(R15-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551176E5)
    (at 240.5 132 315)
    (attr smd)
    (fp_text reference R16 (at -2.520836 -0.060104 495) (layer F.SilkS))
    (fp_text value 47k (at 0 0 315) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(P2-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E4CC7C)
    (at 241.5 131 315)
    (attr smd)
    (fp_text reference R17 (at -2.520836 0.096874 495) (layer F.SilkS))
    (fp_text value 47k (at 0 0 315) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(P2-Pad4)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E4F37B)
    (at 226.06 132.715 180)
    (attr smd)
    (fp_text reference R18 (at 0 -1.397 360) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 IF_AFTER_SAW))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E4F376)
    (at 223.012 132.715 180)
    (attr smd)
    (fp_text reference R19 (at 0 -1.397 360) (layer F.SilkS))
    (fp_text value 1k (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 IF_AFTER_SAW))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D658)
    (at 187.6044 140.5128)
    (attr smd)
    (fp_text reference R20 (at -2.4384 0.0762 180) (layer F.SilkS))
    (fp_text value 50R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(C42-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 542F33AC)
    (at 205.3 127 270)
    (attr smd)
    (fp_text reference R21 (at 3.683 0.068 360) (layer F.SilkS))
    (fp_text value 100R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C51-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 542F33AC)
    (at 205.3 124.5 270)
    (attr smd)
    (fp_text reference R22 (at 5.04 0.068 360) (layer F.SilkS))
    (fp_text value 56R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C54-Pad2)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C51-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 542F33AC)
    (at 205.3 122 90)
    (attr smd)
    (fp_text reference R23 (at 2 0 180) (layer F.SilkS))
    (fp_text value 100R (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C54-Pad2)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 542F33AC)
    (at 239.6 145.8 315)
    (attr smd)
    (fp_text reference R24 (at 0.042426 -1.223295 495) (layer F.SilkS))
    (fp_text value 4k7 (at 0 0 315) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 USB_BOOT))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E4CC81)
    (at 236.061185 138.461185 315)
    (attr smd)
    (fp_text reference R25 (at -0.068589 -1.368252 495) (layer F.SilkS))
    (fp_text value "12k 1%" (at 0 0 315) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0 315) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(R25-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551AD45D)
    (at 245.872 119.888 180)
    (attr smd)
    (fp_text reference R26 (at -0.828 -1.412 360) (layer F.SilkS))
    (fp_text value 4k7 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 RST))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D75C)
    (at 212.6 118.05)
    (attr smd)
    (fp_text reference R27 (at 1.014 -1.21 180) (layer F.SilkS))
    (fp_text value 50R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 IF_AFTER_ATT1))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 542F33AC)
    (at 211.85 120.1 180)
    (attr smd)
    (fp_text reference R29 (at -5.193 -0.042 360) (layer F.SilkS))
    (fp_text value 2k2 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C58-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 542F33AC)
    (at 209.25 120.1 180)
    (attr smd)
    (fp_text reference R30 (at -5.507 -0.042 360) (layer F.SilkS))
    (fp_text value 2k2 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C58-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D77B)
    (at 216.15 124.8 180)
    (attr smd)
    (fp_text reference R32 (at -2.417 -0.041 360) (layer F.SilkS))
    (fp_text value 9R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(C44-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R32-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D796)
    (at 212.05 130.8)
    (attr smd)
    (fp_text reference R33 (at 5.12 -0.879 90) (layer F.SilkS))
    (fp_text value 174R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C61-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R32-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D7A1)
    (at 209.25 130.85 180)
    (attr smd)
    (fp_text reference R35 (at -6.65 0.929 270) (layer F.SilkS))
    (fp_text value 50R (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 IF_AFTER_AMP1))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C61-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551AD24D)
    (at 179.7 127.1 270)
    (attr smd)
    (fp_text reference R36 (at -1.8 -0.1 360) (layer F.SilkS))
    (fp_text value 10R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 LO_SPI_CLOCK))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C78-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 54E0D6AE)
    (at 178.3 128.8 270)
    (attr smd)
    (fp_text reference R37 (at 3.661 0.5 450) (layer F.SilkS))
    (fp_text value 10R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 LO_SPI_DATA))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C79-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_s (layer F.Cu) (tedit 551AD24C)
    (at 179.2 130.7)
    (attr smd)
    (fp_text reference R38 (at -1.2 -4.5 90) (layer F.SilkS))
    (fp_text value 10R (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 21 LO_SPI_LE))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C80-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 55146EC3)
    (at 271.7 130 180)
    (attr smd)
    (fp_text reference R41 (at -0.1 5.5 180) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 55146EC8)
    (at 271.7 128.4 180)
    (attr smd)
    (fp_text reference R42 (at -2.4 4.6 360) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 54E4FBC0)
    (at 180.7 119.4 270)
    (attr smd)
    (fp_text reference R43 (at -0.15 1.45 450) (layer F.SilkS))
    (fp_text value 1k (at -1.69926 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 55103FE3)
    (at 271.9 118.2)
    (attr smd)
    (fp_text reference R44 (at -0.12 2.831 180) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(D5-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 55103FE9)
    (at 271.9 116)
    (attr smd)
    (fp_text reference R45 (at -0.12 3.761 180) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(D6-Pad2)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:LT5560 (layer F.Cu) (tedit 551AD2BD)
    (at 184.4 147.6 90)
    (fp_text reference U3 (at -2.3 1.2 180) (layer F.SilkS))
    (fp_text value LT5560 (at -1.6 0 180) (layer F.SilkS))
    (pad 8 smd rect (at 0.75 1.4125 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C17-Pad1)") (clearance 0.1))
    (pad 7 smd rect (at 0.25 1.4125 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3) (clearance 0.1))
    (pad 6 smd rect (at -0.25 1.4125 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C18-Pad1)") (clearance 0.1))
    (pad 9 smd rect (at 0 0 90) (size 2.38 1.65) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 5 smd rect (at -0.75 1.4125 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C18-Pad2)") (clearance 0.1))
    (pad 4 smd rect (at -0.75 -1.4125 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(B1-Pad4)") (clearance 0.1))
    (pad 3 smd rect (at -0.25 -1.4125 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(B1-Pad3)") (clearance 0.1))
    (pad 2 smd rect (at 0.25 -1.4125 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3) (clearance 0.1))
    (pad 1 smd rect (at 0.75 -1.4125 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(L6-Pad2)") (clearance 0.1))
    (model lib/8dfn3x3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.181 1.181 1.181))
      (rotate (xyz 270 0 0))
    )
  )
  (module mycomponents:so-8 (layer F.Cu) (tedit 5421EFA6)
    (at 213.35 146.15 270)
    (descr SO-8)
    (attr smd)
    (fp_text reference U4 (at 0 -1.016 270) (layer F.SilkS))
    (fp_text value OPA695 (at 0 1.016 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.905 2.794 270) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -0.635 2.794 270) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(R12-Pad2)"))
    (pad 3 smd rect (at 0.635 2.794 270) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C32-Pad1)"))
    (pad 4 smd rect (at 1.905 2.794 270) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at 1.905 -2.794 270) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at 0.635 -2.794 270) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C34-Pad2)"))
    (pad 7 smd rect (at -0.635 -2.794 270) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 8 smd rect (at -1.905 -2.794 270) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model smd/smd_dil/so-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SOT89 (layer F.Cu) (tedit 5421EF1E)
    (at 198.9 140.1 90)
    (fp_text reference U7 (at 0 3 90) (layer F.SilkS))
    (fp_text value MGA-30889 (at 0 0.50038 90) (layer F.SilkS))
    (pad 2 smd trapezoid (at 0 -2.79908 90) (size 1.6002 0.59944) (rect_delta 0 0.59944 ) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance -0.09906))
    (pad 2 smd rect (at 0 -1.39954 270) (size 2.19964 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance -0.09906))
    (pad 2 smd trapezoid (at 0 0.00254 270) (size 1.6002 0.59944) (rect_delta 0 0.59944 ) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance -0.09906))
    (pad 2 smd rect (at 0 1.15062 270) (size 1.00076 1.7018) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance -0.09906))
    (pad 3 smd rect (at 1.50114 1.25222 270) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C48-Pad2)"))
    (pad 1 smd rect (at -1.50114 1.25222 270) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C41-Pad1)"))
    (model lib/sot89.wrl
      (at (xyz 0 0.02 0))
      (scale (xyz 1.673 1.673 1.673))
      (rotate (xyz 270 0 180))
    )
  )
  (module mycomponents:SOT-6 (layer F.Cu) (tedit 5421EF59)
    (at 201.5 127.9 180)
    (descr SOT-6)
    (tags SOT-6)
    (fp_text reference U9 (at 0 0 180) (layer F.SilkS))
    (fp_text value AS169-73 (at 0 -2 180) (layer F.SilkS))
    (pad 2 smd rect (at 0 1.09982 180) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 0.94996 1.09982 180) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C53-Pad2)"))
    (pad 1 smd rect (at -0.94996 1.09982 180) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C51-Pad2)"))
    (pad 5 smd rect (at 0 -1.09982) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C50-Pad1)"))
    (pad 4 smd rect (at 0.94996 -1.09982) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 5 ATT1_SWITCH_B))
    (pad 6 smd rect (at -0.94996 -1.09982) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 4 ATT1_SWITCH_A))
    (model smd/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.122 0.122 0.122))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SF2120C (layer F.Cu) (tedit 55146A05)
    (at 224.0152 142.0912 90)
    (fp_text reference U10 (at -1.9088 3.7848 90) (layer F.SilkS))
    (fp_text value SF2120C (at 0 -1.2 90) (layer F.SilkS))
    (pad 5 smd rect (at 2.015 1.27 90) (size 1.55 0.76) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C55-Pad1)") (clearance 0.1))
    (pad 7 smd rect (at 2.015 -1.27 90) (size 1.55 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 6 smd rect (at 2.015 0 90) (size 1.55 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 2 smd rect (at -2.015 0 90) (size 1.55 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 1 smd rect (at -2.015 -1.27 90) (size 1.55 0.76) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C52-Pad1)") (clearance 0.1))
    (pad 3 smd rect (at -2.015 1.27 90) (size 1.55 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 8 smd rect (at 0 -1.61 90) (size 0.76 2.36) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 4 smd rect (at 0 2.015 90) (size 0.76 1.55) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (model lib/sf2120.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.969 1.969 1.969))
      (rotate (xyz 270 0 0))
    )
  )
  (module mycomponents:SOT-6 (layer F.Cu) (tedit 5421EF59)
    (at 201.5 121.1)
    (descr SOT-6)
    (tags SOT-6)
    (fp_text reference U11 (at 0 0) (layer F.SilkS))
    (fp_text value AS169-73 (at 0 -2) (layer F.SilkS))
    (pad 2 smd rect (at 0 1.09982) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 0.94996 1.09982) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C54-Pad1)"))
    (pad 1 smd rect (at -0.94996 1.09982) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C53-Pad1)"))
    (pad 5 smd rect (at 0 -1.09982 180) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C56-Pad2)"))
    (pad 4 smd rect (at 0.94996 -1.09982 180) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 4 ATT1_SWITCH_A))
    (pad 6 smd rect (at -0.94996 -1.09982 180) (size 0.65024 1.05918) (layers F.Cu F.Paste F.Mask)
      (net 5 ATT1_SWITCH_B))
    (model smd/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.122 0.122 0.122))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:so-8 (layer F.Cu) (tedit 5421EFA6)
    (at 210.65 124.6 180)
    (descr SO-8)
    (attr smd)
    (fp_text reference U13 (at 0 -1.016 180) (layer F.SilkS))
    (fp_text value OPA695 (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.905 2.794 180) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(U13-Pad1)"))
    (pad 2 smd rect (at -0.635 2.794 180) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R32-Pad2)"))
    (pad 3 smd rect (at 0.635 2.794 180) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C58-Pad1)"))
    (pad 4 smd rect (at 1.905 2.794 180) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at 1.905 -2.794 180) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(U13-Pad5)"))
    (pad 6 smd rect (at 0.635 -2.794 180) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C61-Pad2)"))
    (pad 7 smd rect (at -0.635 -2.794 180) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C62-Pad1)"))
    (pad 8 smd rect (at -1.905 -2.794 180) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C62-Pad1)"))
    (model smd/smd_dil/so-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:USB_MICRO_B_FCI (layer F.Cu) (tedit 5422C2BE)
    (at 250.825 115.697 180)
    (clearance 0.1)
    (fp_text reference U14 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value MICRO_USB (at 0 -1.65 180) (layer F.SilkS))
    (pad 5 smd rect (at 1.3 -2.85 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 4 smd rect (at 0.65 -2.85 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(U14-Pad4)"))
    (pad 3 smd rect (at 0 -2.85 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(U14-Pad3)"))
    (pad 2 smd rect (at -0.65 -2.85 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(U14-Pad2)"))
    (pad 1 smd rect (at -1.3 -2.85 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 25 VCC))
    (pad 6 smd rect (at 1.15 0 180) (size 1.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 6 smd rect (at -1.15 0 180) (size 1.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 6 smd rect (at 3.75 0 180) (size 2.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 6 smd rect (at -3.75 0 180) (size 2.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model lib/AB2_USB_MICRO_SMD.wrl
      (at (xyz 0 -0.105 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:TO252 (layer F.Cu) (tedit 54E4C80D)
    (at 226.187 156.337 90)
    (fp_text reference U15 (at -2.667 3.048 180) (layer F.SilkS))
    (fp_text value 78M33 (at 0 -9.5 90) (layer F.SilkS))
    (pad GND smd rect (at 0 -6.9 90) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad VO smd rect (at 2.3 0 90) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad VI smd rect (at -2.3 0 90) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
  )
  (module mycomponents:TO252 (layer F.Cu) (tedit 551177F9)
    (at 209.423 156.337 90)
    (fp_text reference U16 (at -2.667 3.048 180) (layer F.SilkS))
    (fp_text value 78L05 (at 0 -9.5 90) (layer F.SilkS))
    (pad GND smd rect (at 0 -6.9 90) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad VO smd rect (at 2.3 0 90) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad VI smd rect (at -2.3 0 90) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 54E4F988)
    (at 195 158.5 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at -1 -1 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D7-Pad2)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 551A92D3)
    (at 274.7 126.8 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at -4.899 2.997 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(D8-Pad2)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 55117722)
    (at 197 120.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at -0.027 1.374 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.016 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 ATT1_SWITCH_B))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(D9-Pad2)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 551ACF4F)
    (at 236.22 149.733)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D10 (at 2.78 0.067) (layer F.SilkS))
    (fp_text value LED (at 0 1.016) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 551A92DD)
    (at 274.7 131.6 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D11 (at -6.699 -0.401 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.016 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D11-Pad2)"))
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 54E4F98E)
    (at 192 158.5 180)
    (attr smd)
    (fp_text reference R48 (at 2.5 0 360) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 55146EC6)
    (at 271.7 126.8 180)
    (attr smd)
    (fp_text reference R49 (at -0.1 3.6 360) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 55117724)
    (at 197 117.5 90)
    (attr smd)
    (fp_text reference R50 (at -0.229 1.374 270) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 5512BAD8)
    (at 233.172 149.733)
    (attr smd)
    (fp_text reference R51 (at -2.472 -0.033 180) (layer F.SilkS))
    (fp_text value 220R (at -1.69926 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 206 /TCAL_EN))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(D10-Pad1)"))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:SM0603_Resistor_s (layer F.Cu) (tedit 55146EC0)
    (at 271.7 131.6 180)
    (attr smd)
    (fp_text reference R52 (at -2.4 6.5 360) (layer F.SilkS))
    (fp_text value 4k7 (at -1.69926 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:FOX924B (layer F.Cu) (tedit 55146E46)
    (at 188 118 180)
    (fp_text reference X1 (at -4.2 1.7 180) (layer F.SilkS))
    (fp_text value TCXO (at 0.635 -3.175 180) (layer F.Fab))
    (pad 4 smd rect (at -2 -1.25 180) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 3 smd rect (at 2 -1.25 180) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C28-Pad1)"))
    (pad 1 smd rect (at -2 1.25 180) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 2 smd rect (at 2 1.25 180) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
  )
  (module mycomponents:FOX924B (layer F.Cu) (tedit 5511762D)
    (at 267.208 124.46 270)
    (fp_text reference X3 (at -1.397 3.175 270) (layer F.SilkS))
    (fp_text value TCXO (at 0.635 -3.175 270) (layer F.Fab))
    (pad 4 smd rect (at -2 -1.25 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 3 smd rect (at 2 -1.25 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(U5-Pad120)"))
    (pad 1 smd rect (at -2 1.25 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 2 1.25 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
  )
  (module mycomponents:sot23 (layer F.Cu) (tedit 55146419)
    (at 223.8652 149.0412 270)
    (descr SOT23)
    (attr smd)
    (fp_text reference U18 (at 1.4088 -2.3848 360) (layer F.SilkS))
    (fp_text value LIMITER_DIODE (at 0 2.3 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 IF_AFTER_AMP2))
    (pad 2 smd rect (at 0 -1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 0.9525 1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 IF_AFTER_AMP2))
    (model Transistors_SMD/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:sot23 (layer F.Cu) (tedit 54E4F35A)
    (at 222.6 130.1 90)
    (descr SOT23)
    (attr smd)
    (fp_text reference U17 (at -0.9 3 180) (layer F.SilkS))
    (fp_text value LIMITER_DIODE (at 0 2.3 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 13 IF_AFTER_SAW))
    (pad 2 smd rect (at 0 -1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(C40-Pad1)"))
    (pad 3 smd rect (at 0.9525 1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 13 IF_AFTER_SAW))
    (model Transistors_SMD/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:micromatch_4 (layer F.Cu) (tedit 54E4FC9E)
    (at 245.2 156.1)
    (fp_text reference P5 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 198 /TRIG_CONNECTED))
    (pad 2 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 199 /TRIG_INT))
    (pad 3 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 200 /TRIG_OUT))
    (pad 4 thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad "" thru_hole circle (at 2.67 0.53) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module mycomponents:micromatch_4 (layer F.Cu) (tedit 54E4FC9E)
    (at 235.7 156.1)
    (fp_text reference P4 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 195 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 196 "Net-(P4-Pad3)"))
    (pad 4 thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 197 "Net-(P4-Pad4)"))
    (pad "" thru_hole circle (at 2.67 0.53) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 223.5 119.5 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C49 (at 0.1 -1.8 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mycomponents:3SOT223 (layer F.Cu) (tedit 5515648C)
    (at 226.275 118.4 270)
    (fp_text reference U19 (at 2.5 -7.225 450) (layer F.SilkS))
    (fp_text value LM2937IMP-3.3 (at -1.27 1.905 270) (layer F.Fab))
    (pad GND smd rect (at 0 -4.725 270) (size 3.25 2.15) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad VI smd rect (at -2.3 0 270) (size 0.95 2.15) (layers F.Cu F.Paste F.Mask)
      (net 25 VCC))
    (pad GND smd rect (at 0 0 270) (size 0.95 2.15) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad VO smd rect (at 2.3 0 270) (size 0.95 2.15) (layers F.Cu F.Paste F.Mask)
      (net 207 +3.3VADC))
  )
  (module mycomponents:LFCSP-32-2 (layer F.Cu) (tedit 551AD257)
    (at 186.07 131.31)
    (tags LFCSP-32-2)
    (clearance 0.1)
    (fp_text reference U1 (at -3.27 3.19) (layer F.SilkS))
    (fp_text value ADF4350 (at 0 0) (layer F.SilkS))
    (pad 33 smd rect (at 0 0) (size 3.0988 3.0988) (layers F.Cu F.Mask)
      (net 7 GND))
    (pad 8 smd rect (at -2.32918 1.74498) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 7 smd rect (at -2.33172 1.2446) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 6 CP_OUT))
    (pad 6 smd rect (at -2.33172 0.74422) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 5 smd rect (at -2.33172 0.24638) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -2.33172 -0.254) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 3 smd rect (at -2.33172 -0.75438) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C80-Pad2)"))
    (pad 2 smd rect (at -2.33172 -1.25476) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C79-Pad2)"))
    (pad 1 smd rect (at -2.33172 -1.75514) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C78-Pad2)"))
    (pad 24 smd rect (at 2.32918 -1.75006) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C11-Pad1)"))
    (pad 23 smd rect (at 2.33172 -1.2319) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C13-Pad1)"))
    (pad 22 smd rect (at 2.33172 -0.73152) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(R4-Pad2)"))
    (pad 21 smd rect (at 2.33172 -0.23114) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 20 smd rect (at 2.33172 0.2667) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 26 V_TUNE))
    (pad 19 smd rect (at 2.33172 0.76708) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C15-Pad1)"))
    (pad 18 smd rect (at 2.33172 1.26746) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 17 smd rect (at 2.33172 1.76784) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 29 smd rect (at -0.25146 -2.32918 90) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 16 LO_CLOCK))
    (pad 28 smd rect (at 0.24892 -2.32918 90) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 27 smd rect (at 0.7493 -2.32918 90) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 26 smd rect (at 1.24968 -2.32918 90) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 30 smd rect (at -0.75184 -2.32918 90) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at -1.25222 -2.32918 90) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 32 smd rect (at -1.7526 -2.32918 90) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 12 smd rect (at -0.25146 2.32918 270) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C6-Pad2)"))
    (pad 13 smd rect (at 0.24892 2.32918 270) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(C42-Pad2)"))
    (pad 14 smd rect (at 0.7493 2.32918 270) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.24968 2.32918 270) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U1-Pad15)"))
    (pad 11 smd rect (at -0.75184 2.32918 270) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 10 smd rect (at -1.25222 2.32918 270) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 9 smd rect (at -1.75006 2.32918 270) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 16 smd rect (at 1.75006 2.32918 270) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 215 +3V3))
    (pad 25 smd rect (at 1.7526 -2.32918 90) (size 0.58928 0.28) (layers F.Cu F.Paste F.Mask)
      (net 17 LO_LOCK_DETECT))
    (pad ~ smd rect (at -0.8 -0.8) (size 1.15 1.15) (layers F.Paste))
    (pad ~ smd rect (at 0.8 -0.8) (size 1.15 1.15) (layers F.Paste))
    (pad ~ smd rect (at -0.8 0.8) (size 1.15 1.15) (layers F.Paste))
    (pad ~ smd rect (at 0.8 0.8) (size 1.15 1.15) (layers F.Paste))
    (model lib/lfcsp32.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.97 1.97 1.97))
      (rotate (xyz 270 0 0))
    )
  )
  (module mycomponents:SMA_SIDE (layer F.Cu) (tedit 551AFA2F)
    (at 183 157.5 180)
    (fp_text reference P1 (at 0 3.2 180) (layer F.SilkS) hide)
    (fp_text value BNC (at 0 3.8 180) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 2.5 5) (layers F.Cu F.Mask)
      (net 32 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -3.5 0 180) (size 3 5) (layers *.Mask B.Cu)
      (net 7 GND))
    (pad 2 smd rect (at 3.5 0 180) (size 3 5) (layers F.Cu F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 3.5 0 180) (size 3 5) (layers *.Mask B.Cu)
      (net 7 GND))
    (pad 2 smd rect (at -3.5 0 180) (size 3 5) (layers F.Cu F.Mask)
      (net 7 GND))
    (model lib/SMA_EDGE.wrl
      (at (xyz -0 0.15 0.063))
      (scale (xyz 1.27 1.27 1.27))
      (rotate (xyz 90 0 90))
    )
  )
  (gr_text "Rev. 2" (at 235.4 142.6 90) (layer F.SilkS))
  (gr_text "5V0\n\n" (at 269.3 129) (layer F.SilkS))
  (gr_text "3V3A\n" (at 268.9 131.7) (layer F.SilkS))
  (gr_text "Att 20dB" (at 197 126.5 90) (layer F.SilkS))
  (gr_text OVERLOAD (at 193 156.75) (layer F.SilkS))
  (gr_text 3V3 (at 226.314 155.829) (layer F.SilkS))
  (gr_text 5V (at 209.423 155.829) (layer F.SilkS))
  (gr_text TRIG (at 244.9 152) (layer F.SilkS))
  (gr_text TCAL (at 235.5 152) (layer F.SilkS))
  (gr_text "LPC 4333" (at 256.5 154.5) (layer F.SilkS))
  (gr_text "8-15 VDC IN" (at 263.1 155.5 90) (layer F.SilkS))
  (gr_line (start 277 160) (end 177 160) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 277 114.3) (end 277 160) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177 114.27) (end 277 114.27) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177 160) (end 177 114.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "21cm HI Receiver\nSven Brauch 2015" (at 232.5 139.75 90) (layer F.SilkS))
  (gr_text S2 (at 269.9 118.3) (layer F.SilkS))
  (gr_text S1 (at 269.9 116) (layer F.SilkS))
  (gr_text "3V3\n" (at 269.3 130) (layer F.SilkS))
  (gr_text "LO\nLOCK" (at 181.3 116.8) (layer F.SilkS))
  (gr_text . (at 275.2 133.8) (layer F.SilkS))
  (gr_text ISP (at 273.1 142.6) (layer F.SilkS))
  (gr_text . (at 232.75 115.25 90) (layer F.SilkS))
  (gr_text JTAG (at 241.75 117.5 90) (layer F.SilkS))
  (zone (net 7) (net_name GND) (layer Inner2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 277 160) (xy 184.9 160) (xy 177 160) (xy 177 154.5) (xy 177 142.5)
        (xy 177 141.5) (xy 177 133.5) (xy 177 113) (xy 277 113) (xy 277 159)
        (xy 277 160)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179 141.5) (xy 181.5 141.5) (xy 181.5 142.5) (xy 179 142.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177 154.5) (xy 188 154.5) (xy 188 155.5) (xy 177 155.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 197.5 149) (xy 198.5 149) (xy 198.5 151) (xy 197.5 151)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.5 137.5) (xy 213.5 138.5) (xy 215.5 138.5) (xy 215.5 137.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.9652 149.6412) (xy 224.9652 150.6412) (xy 221.9652 150.6412) (xy 221.9652 149.6412)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 202.5 131.5) (xy 204 131.5) (xy 204 132.5) (xy 202.5 132.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 206.5 116.5) (xy 207.5 116.5) (xy 207.5 119) (xy 207.5 119.5) (xy 206.5 119.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Inner2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205 120) (xy 206 120) (xy 206 160) (xy 205 160) (xy 205 121)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Inner2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 218.5 142.5) (xy 218 142.5) (xy 217.5 142.5) (xy 217.5 113) (xy 218.5 113)
        (xy 218.5 140.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Inner2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 230.5 160) (xy 230.5 131) (xy 229.5 131) (xy 229.5 160)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177 125) (xy 178.5 125) (xy 178.5 133.5) (xy 177 133.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.026)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 217.5 137.5) (xy 218.5 137.5) (xy 218.5 138.5) (xy 217.5 138.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.026)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.5 154.5) (xy 177 154.5) (xy 177 133.5) (xy 178.5 133.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.026)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 229.5 152.5) (xy 198.5 152.5) (xy 198.5 155.5) (xy 188 155.5) (xy 188 154.5)
        (xy 197.5 154.5) (xy 197.5 151) (xy 198.5 151) (xy 198.5 151.5) (xy 206.5 151.5)
        (xy 206.5 144.5) (xy 206.5 144.5) (xy 206.5 143.5) (xy 206.5 143.5) (xy 206.5 132.5)
        (xy 206.5 132.5) (xy 206.5 131.5) (xy 206.5 131.5) (xy 206.5 119.5) (xy 207.5 119.5)
        (xy 207.5 131.5) (xy 207.5 131.5) (xy 207.5 132.5) (xy 207.5 132.5) (xy 207.5 137.5)
        (xy 213.5 137.5) (xy 213.5 138.5) (xy 207.5 138.5) (xy 207.5 151.5) (xy 228.5 151.5)
        (xy 228.5 138.5) (xy 226.7 138.5) (xy 226.7 137.5) (xy 229.5 137.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.026)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 221.5 138.5) (xy 220.5 138.5) (xy 220.5 150) (xy 219.5 150) (xy 219.5 138.5)
        (xy 215.5 138.5) (xy 215.5 137.5) (xy 219.5 137.5) (xy 219.5 132.5) (xy 216 132.5)
        (xy 216 131.5) (xy 219.5 131.5) (xy 219.5 115.5) (xy 195.5 115.5) (xy 195.5 131.5)
        (xy 202 131.5) (xy 202 132.5) (xy 195.5 132.5) (xy 195.5 143.5) (xy 198.5 143.5)
        (xy 198.5 149) (xy 197.5 149) (xy 197.5 144.5) (xy 194.5 144.5) (xy 194.5 142.5)
        (xy 181.5 142.5) (xy 181.5 141.5) (xy 194.5 141.5) (xy 194.5 115.5) (xy 178.5 115.5)
        (xy 178.5 125) (xy 177 125) (xy 177 114) (xy 220.5 114) (xy 220.5 137.5)
        (xy 221.5 137.5)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 277 113) (xy 177 113) (xy 177 160) (xy 277 160)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 208.5 133) (xy 236.5 133) (xy 236.5 135) (xy 208.5 135) (xy 208.5 134.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 189.5 126.5) (xy 192.5 126.5) (xy 192.5 129.5) (xy 189.5 129.5)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer Inner1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 228 151) (xy 199 151) (xy 199 143) (xy 197 143) (xy 197 123)
        (xy 196 123) (xy 196 114.5) (xy 218.5 114.5) (xy 218.5 139) (xy 228 139)
      )
    )
  )
  (zone (net 215) (net_name +3V3) (layer Inner1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177 114.3) (xy 195.3 114.2) (xy 195.3 123.9) (xy 196.1 123.9) (xy 196.1 131.9)
        (xy 195.6 131.9) (xy 195.6 142.6) (xy 195.6 144.6) (xy 197.3 144.6) (xy 197.3 151)
        (xy 177 151) (xy 176.9 151)
      )
    )
  )
  (zone (net 207) (net_name +3.3VADC) (layer Inner1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 277 157.9) (xy 230 157.9) (xy 230 137) (xy 219.5 137) (xy 219.5 114.5)
        (xy 277 114.5)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 221.5 138.5) (xy 220.5 138.5) (xy 220.5 150) (xy 219.5 150) (xy 219.5 138.5)
        (xy 218.5 138.5) (xy 218.5 137.5) (xy 219.5 137.5) (xy 219.5 132.5) (xy 211 132.5)
        (xy 211 131.5) (xy 219.5 131.5) (xy 219.5 115.5) (xy 195.5 115.5) (xy 195.5 131.5)
        (xy 202 131.5) (xy 202 132.5) (xy 195.5 132.5) (xy 195.5 143.5) (xy 198.5 143.5)
        (xy 198.5 149) (xy 197.5 149) (xy 197.5 144.5) (xy 194.5 144.5) (xy 194.5 142.5)
        (xy 181.5 142.5) (xy 181.5 141.5) (xy 194.5 141.5) (xy 194.5 115.5) (xy 178.5 115.5)
        (xy 178.5 125) (xy 176.5 125) (xy 176.5 115) (xy 176.5 113.5) (xy 177 113.5)
        (xy 220.5 113.5) (xy 220.5 137.5) (xy 221.5 137.5)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.5 154.5) (xy 178.5 133.5) (xy 177 133.5) (xy 177 154.5)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 229.5 152.5) (xy 198.5 152.5) (xy 198.5 155.5) (xy 188 155.5) (xy 188 154.5)
        (xy 197.5 154.5) (xy 197.5 151) (xy 198.5 151) (xy 198.5 151.5) (xy 206.5 151.5)
        (xy 206.5 119.5) (xy 207.5 119.5) (xy 207.5 137.5) (xy 213.5 137.5) (xy 213.5 138.5)
        (xy 209.5 138.5) (xy 209.5 151.5) (xy 228.5 151.5) (xy 228.5 138.5) (xy 226.8 138.5)
        (xy 226.8 137.5) (xy 229.5 137.5)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.5 137.5) (xy 217.5 137.5) (xy 217.5 138.5) (xy 215.5 138.5)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 202.5 143.5) (xy 205.5 143.5) (xy 205.5 144.5) (xy 202.5 144.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 210.1 151.5) (xy 213.4 151.5) (xy 213.4 152.1) (xy 210.1 152.1)
      )
    )
  )
)
